Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package org.teleal.cling.model.message.header

Class Summary
CallbackHeader |
ContentTypeHeader |
DeviceTypeHeader |
DeviceUSNHeader |
EventSequenceHeader |
EXTHeader |
HostHeader |
InterfaceMacHeader | Extension header, allows us to transfer the MAC ethernet address for Wake-on-LAN.
LocationHeader | TODO: UDA 1.1 says it should be RfC 3986 compatible: http://blog.jclark.com/2008/11/what-allowed-in-uri.html
MANHeader | Another experimental and pointless Microsoft RFC 2774!
MaxAgeHeader |
MXHeader |
NTEventHeader |
NTSHeader |
RootDeviceHeader |
ServerHeader |
ServiceTypeHeader |
ServiceUSNHeader |
SoapActionHeader | Needs to also parse: "urn:schemas-upnp-org:control-1-0#QueryStateVariable"
STAllHeader |
SubscriptionIdHeader |
TimeoutHeader |
UDADeviceTypeHeader |
UDAServiceTypeHeader |
UDNHeader |
UpnpHeader<T> |
UserAgentHeader |
USNRootDeviceHeader |

Enum Summary
UpnpHeader.Type |

Exception Summary
InvalidHeaderException |

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

Copyright © 2010 Teleal GmbH, Switzerland. All Rights Reserved.