Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## org.teleal.cling.transport.spi
Interface MulticastReceiverConfiguration

All Known Implementing Classes:
  MulticastReceiverConfigurationImpl

    public interface MulticastReceiverConfiguration

Collection of typically needed configuration settings.

Author:
  Christian Bauer

Method Summary
`InetAddress` | `getGroup()`
`int` | `getMaxDatagramBytes()`
`int` | `getPort()`

Method Detail

### getGroup

    InetAddress getGroup()

  Returns:
    The multicast group to join.

### getPort

    int getPort()

  Returns:
    The port to listen on.

### getMaxDatagramBytes

    int getMaxDatagramBytes()

  Returns:
    The maximum buffer size of received UDP datagrams.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

Copyright © 2010 Teleal GmbH, Switzerland. All Rights Reserved.