Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package org.teleal.cling.model.types

Interface Summary
Datatype<V> | The type of a state variable value, able to convert to/from string representation.

Class Summary
AbstractDatatype<V> |
Base64Datatype |
BinHexDatatype |
BooleanDatatype |
CharacterDatatype |
CustomDatatype |
DateTimeDatatype |
DeviceType | Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
DLNACaps | An arbitrary list of comma-separated elements, representing DLNA capabilities (whatever that is).
DLNADoc | Representing the DLNA document and its version.
DoubleDatatype |
FloatDatatype |
HostPort | Encapsulates a host string and a port.
IntegerDatatype | Although the UDA 1.0 spec doesn't say it, we assume that "int" is a 4 byte regular Java integer.
NamedDeviceType | Combines a `UDN` with a `DeviceType`, string representation is separated by double-colon.
NamedServiceType | Combines a `UDN` with a `ServiceType`, string representation is separated by double-colon.
ServiceId | Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
ServiceType | Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
SoapActionType | Header in SOAP action messages, naturally declaring the same thing as the body of the SOAP message.
StringDatatype |
TimeDatatype |
UDADeviceType | Device type with a fixed `schemas-upnp-org` namespace.
UDAServiceId | Service identifier with a fixed `upnp-org` namespace.
UDAServiceType | Service type with a fixed `schemas-upnp-org` namespace.
UDN | A unique device name.
UnsignedIntegerFourBytes |
UnsignedIntegerFourBytesDatatype |
UnsignedIntegerOneByte |
UnsignedIntegerOneByteDatatype |
UnsignedIntegerTwoBytes |
UnsignedIntegerTwoBytesDatatype |
UnsignedVariableInteger | A crude solution for unsigned "non-negative" types in UPnP, not usable for any arithmetic.
URIDatatype |

Enum Summary
Datatype.Builtin | Mapping from UPnP built-in standardized type to actual subtype of `Datatype`.
Datatype.Default | Mapping from Java type to UPnP built-in type.
DLNADoc.Version |
ErrorCode | Basic UPnP control message error codes.
NotificationSubtype | Notification message types for SSDP.
UnsignedVariableInteger.Bits |

Exception Summary
InvalidValueException | Thrown by datatypes and variable value conversion procedures.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

Copyright © 2010 Teleal GmbH, Switzerland. All Rights Reserved.