Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## org.teleal.cling.transport.impl
Class MulticastReceiverConfigurationImpl

    java.lang.Object
      org.teleal.cling.transport.impl.MulticastReceiverConfigurationImpl

All Implemented Interfaces:
  MulticastReceiverConfiguration

    public class MulticastReceiverConfigurationImpl

extends Object
implements MulticastReceiverConfiguration

Settings for the default implementation.

Author:
  Christian Bauer

Constructor Summary
`MulticastReceiverConfigurationImpl(InetAddress group, int port)` Defaults to maximum datagram size of 640 bytes (512 per UDA 1.0, 128 byte header).
`MulticastReceiverConfigurationImpl(InetAddress group, int port, int maxDatagramBytes)`
`MulticastReceiverConfigurationImpl(String group, int port)` Defaults to maximum datagram size of 640 bytes (512 per UDA 1.0, 128 byte header).
`MulticastReceiverConfigurationImpl(String group, int port, int maxDatagramBytes)`

Method Summary
`InetAddress` | `getGroup()`
`int` | `getMaxDatagramBytes()`
`int` | `getPort()`
`void` | `setGroup(InetAddress group)`
`void` | `setMaxDatagramBytes(int maxDatagramBytes)`
`void` | `setPort(int port)`

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Constructor Detail

### MulticastReceiverConfigurationImpl

    public MulticastReceiverConfigurationImpl(InetAddress group,
                                              int port,
                                              int maxDatagramBytes)

### MulticastReceiverConfigurationImpl

    public MulticastReceiverConfigurationImpl(InetAddress group,
                                              int port)

  Defaults to maximum datagram size of 640 bytes (512 per UDA 1.0, 128 byte header).

### MulticastReceiverConfigurationImpl

    public MulticastReceiverConfigurationImpl(String group,
                                              int port,
                                              int maxDatagramBytes)
                                       throws UnknownHostException

Throws:
  `UnknownHostException`

### MulticastReceiverConfigurationImpl

    public MulticastReceiverConfigurationImpl(String group,
                                              int port)
                                       throws UnknownHostException

  Defaults to maximum datagram size of 640 bytes (512 per UDA 1.0, 128 byte header).

  Throws:
    `UnknownHostException`

Method Detail

### getGroup

    public InetAddress getGroup()

  Specified by:
    `getGroup` in interface `MulticastReceiverConfiguration`
  Returns:
    The multicast group to join.

### setGroup

    public void setGroup(InetAddress group)

### getPort

    public int getPort()

  Specified by:
    `getPort` in interface `MulticastReceiverConfiguration`
  Returns:
    The port to listen on.

### setPort

    public void setPort(int port)

### getMaxDatagramBytes

    public int getMaxDatagramBytes()

  Specified by:
    `getMaxDatagramBytes` in interface `MulticastReceiverConfiguration`
  Returns:
    The maximum buffer size of received UDP datagrams.

### setMaxDatagramBytes

    public void setMaxDatagramBytes(int maxDatagramBytes)

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

Copyright © 2010 Teleal GmbH, Switzerland. All Rights Reserved.