Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Interface
org.teleal.cling.model.Validatable

Packages that use Validatable
org.teleal.cling.model.meta |

Uses of Validatable in org.teleal.cling.model.meta

Classes in org.teleal.cling.model.meta that implement Validatable
`class` | `Action<S extends Service>` Describes an action and its input/output arguments.
`class` | `ActionArgument<S extends Service>` Describes a single action argument, either input or output.
`class` | `Device<DI extends DeviceIdentity,D extends Device,S extends Service>` Describes either a root or embedded device.
`class` | `DeviceDetails` Encapsulates all optional metadata about a device.
`class` | `Icon` The metadata of a device icon, might include the actual image data of a local icon.
`class` | `LocalDevice` The metadata of a device created on this host, by application code.
`class` | `QueryStateVariableAction<S extends Service>` Describes a single action, the deprecated "query any state variable" action.
`class` | `RemoteDevice` The metadata of a device that was discovered on the network.
`class` | `StateVariable<S extends Service>` The metadata of a named state variable.
`class` | `StateVariableAllowedValueRange` Integrity rule for a state variable, restricting its values to a range with steps.
`class` | `StateVariableTypeDetails` Type of a state variable, its default value, and integrity rules for allowed values and ranges.
`class` | `UDAVersion` Version of the UPnP Device Architecture (UDA), defaults to 1.0.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Copyright © 2010 Teleal GmbH, Switzerland. All Rights Reserved.