Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package org.teleal.cling.transport.spi

Interface Summary
DatagramIO<C extends DatagramIOConfiguration> | Service for receiving (unicast only) and sending UDP datagrams, one per bound IP address.
DatagramIOConfiguration | Collection of typically needed configuration settings.
DatagramProcessor | Reads and creates UDP datagrams from and into UPnP messages.
GENAEventProcessor | Reads and writes GENA XML content.
MulticastReceiver<C extends MulticastReceiverConfiguration> | Service for receiving multicast UDP datagrams, one per bound network interface.
MulticastReceiverConfiguration | Collection of typically needed configuration settings.
NetworkAddressFactory | Configuration utility for network interfaces and addresses.
SOAPActionProcessor | Converts UPnP SOAP messages from/to action invocations.
StreamClient<C extends StreamClientConfiguration> | Service for sending TCP (HTTP) stream request messages.
StreamClientConfiguration | Collection of typically needed configuration settings.
StreamServer<C extends StreamServerConfiguration> | Service for receiving TCP (HTTP) streams, one per bound IP address.
StreamServerConfiguration | Collection of typically needed configuration settings.

Class Summary
UpnpStream | A runnable representation of a single HTTP request/response procedure.

Exception Summary
InitializationException | Thrown by the transport layer implementation when service setup fails.
UnsupportedDataException | Thrown by processors/converters when errors occured.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

Copyright © 2011 Teleal GmbH, Switzerland. All Rights Reserved.