Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Package
org.teleal.cling.model.types

Packages that use org.teleal.cling.model.types
org.teleal.cling |
org.teleal.cling.binding |
org.teleal.cling.binding.annotations |
org.teleal.cling.binding.staging |
org.teleal.cling.model |
org.teleal.cling.model.action |
org.teleal.cling.model.gena |
org.teleal.cling.model.message.discovery |
org.teleal.cling.model.message.gena |
org.teleal.cling.model.message.header |
org.teleal.cling.model.meta |
org.teleal.cling.model.state |
org.teleal.cling.model.types |
org.teleal.cling.model.types.csv |
org.teleal.cling.protocol.async |
org.teleal.cling.protocol.sync |
org.teleal.cling.registry |

Classes in org.teleal.cling.model.types used by org.teleal.cling
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.

Classes in org.teleal.cling.model.types used by org.teleal.cling.binding
ServiceId Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.

Classes in org.teleal.cling.model.types used by org.teleal.cling.binding.annotations
Datatype The type of a state variable value, able to convert to/from string representation.
ServiceId Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.

Classes in org.teleal.cling.model.types used by org.teleal.cling.binding.staging
Datatype The type of a state variable value, able to convert to/from string representation.
DeviceType Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
DLNACaps An arbitrary list of comma-separated elements, representing DLNA capabilities (whatever that is).
DLNADoc Representing the DLNA document and its version.
ServiceId Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
UDN A unique device name.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model
Datatype The type of a state variable value, able to convert to/from string representation.
InvalidValueException Thrown by datatypes and variable value conversion procedures.
ServiceId Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
UDN A unique device name.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.action
ErrorCode Basic UPnP control message error codes.
InvalidValueException Thrown by datatypes and variable value conversion procedures.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.gena
UnsignedIntegerFourBytes

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.message.discovery
NotificationSubtype Notification message types for SSDP.
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
UDN A unique device name.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.message.gena
UnsignedIntegerFourBytes

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.message.header
DeviceType Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
NamedDeviceType Combines a `UDN` with a `DeviceType`, string representation is separated by double-colon.
NamedServiceType Combines a `UDN` with a `ServiceType`, string representation is separated by double-colon.
NotificationSubtype Notification message types for SSDP.
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
SoapActionType Header in SOAP action messages, naturally declaring the same thing as the body of the SOAP message.
UDAServiceType Service type with a fixed `schemas-upnp-org` namespace.
UDN A unique device name.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.meta
Datatype The type of a state variable value, able to convert to/from string representation.
DeviceType Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
DLNACaps An arbitrary list of comma-separated elements, representing DLNA capabilities (whatever that is).
DLNADoc Representing the DLNA document and its version.
ServiceId Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
UDN A unique device name.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.state
InvalidValueException Thrown by datatypes and variable value conversion procedures.

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.types
AbstractDatatype
Datatype The type of a state variable value, able to convert to/from string representation.
Datatype.Builtin Mapping from UPnP built-in standardized type to actual subtype of `Datatype`.
Datatype.Default Mapping from Java type to UPnP built-in type.
DeviceType Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
DLNACaps An arbitrary list of comma-separated elements, representing DLNA capabilities (whatever that is).
DLNADoc Representing the DLNA document and its version.
DLNADoc.Version
ErrorCode Basic UPnP control message error codes.
InvalidValueException Thrown by datatypes and variable value conversion procedures.
NamedDeviceType Combines a `UDN` with a `DeviceType`, string representation is separated by double-colon.
NamedServiceType Combines a `UDN` with a `ServiceType`, string representation is separated by double-colon.
NotificationSubtype Notification message types for SSDP.
ServiceId Represents a service identifer, for example `urn:my-domain-namespace:serviceId:MyService123`
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
SoapActionType Header in SOAP action messages, naturally declaring the same thing as the body of the SOAP message.
UDADeviceType Device type with a fixed `schemas-upnp-org` namespace.
UDAServiceId Service identifier with a fixed `upnp-org` namespace.
UDAServiceType Service type with a fixed `schemas-upnp-org` namespace.
UDN A unique device name.
UnsignedIntegerFourBytes
UnsignedIntegerOneByte
UnsignedIntegerTwoBytes
UnsignedVariableInteger A crude solution for unsigned "non-negative" types in UPnP, not usable for any arithmetic.
UnsignedVariableInteger.Bits

Classes in org.teleal.cling.model.types used by org.teleal.cling.model.types.csv
Datatype.Builtin Mapping from UPnP built-in standardized type to actual subtype of `Datatype`.
InvalidValueException Thrown by datatypes and variable value conversion procedures.

Classes in org.teleal.cling.model.types used by org.teleal.cling.protocol.async
DeviceType Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
NotificationSubtype Notification message types for SSDP.
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
UDN A unique device name.

Classes in org.teleal.cling.model.types used by org.teleal.cling.protocol.sync
UnsignedIntegerFourBytes

Classes in org.teleal.cling.model.types used by org.teleal.cling.registry
DeviceType Represents a device type, for example `urn:my-domain-namespace:device:MyDevice:1`.
ServiceType Represents a service type, for example `urn:my-domain-namespace:service:MyService:1`.
UDN A unique device name.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Copyright © 2011 Teleal GmbH, Switzerland. All Rights Reserved.