Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Package
org.teleal.cling.transport.spi

Packages that use org.teleal.cling.transport.spi
org.teleal.cling |
org.teleal.cling.android |
org.teleal.cling.mock |
org.teleal.cling.transport |
org.teleal.cling.transport.impl |
org.teleal.cling.transport.impl.apache |
org.teleal.cling.transport.spi |

Classes in org.teleal.cling.transport.spi used by org.teleal.cling
DatagramIO Service for receiving (unicast only) and sending UDP datagrams, one per bound IP address.
DatagramProcessor Reads and creates UDP datagrams from and into UPnP messages.
GENAEventProcessor Reads and writes GENA XML content.
MulticastReceiver Service for receiving multicast UDP datagrams, one per bound network interface.
NetworkAddressFactory Configuration utility for network interfaces and addresses.
SOAPActionProcessor Converts UPnP SOAP messages from/to action invocations.
StreamClient Service for sending TCP (HTTP) stream request messages.
StreamServer Service for receiving TCP (HTTP) streams, one per bound IP address.

Classes in org.teleal.cling.transport.spi used by org.teleal.cling.android
InitializationException Thrown by the transport layer implementation when service setup fails.
NetworkAddressFactory Configuration utility for network interfaces and addresses.
StreamClient Service for sending TCP (HTTP) stream request messages.
StreamServer Service for receiving TCP (HTTP) streams, one per bound IP address.

Classes in org.teleal.cling.transport.spi used by org.teleal.cling.mock
NetworkAddressFactory Configuration utility for network interfaces and addresses.
StreamClient Service for sending TCP (HTTP) stream request messages.
UpnpStream A runnable representation of a single HTTP request/response procedure.

Classes in org.teleal.cling.transport.spi used by org.teleal.cling.transport
DatagramIO Service for receiving (unicast only) and sending UDP datagrams, one per bound IP address.
InitializationException Thrown by the transport layer implementation when service setup fails.
MulticastReceiver Service for receiving multicast UDP datagrams, one per bound network interface.
NetworkAddressFactory Configuration utility for network interfaces and addresses.
StreamClient Service for sending TCP (HTTP) stream request messages.
StreamServer Service for receiving TCP (HTTP) streams, one per bound IP address.
UpnpStream A runnable representation of a single HTTP request/response procedure.

Classes in org.teleal.cling.transport.spi used by org.teleal.cling.transport.impl
DatagramIO Service for receiving (unicast only) and sending UDP datagrams, one per bound IP address.
DatagramIOConfiguration Collection of typically needed configuration settings.
DatagramProcessor Reads and creates UDP datagrams from and into UPnP messages.
GENAEventProcessor Reads and writes GENA XML content.
InitializationException Thrown by the transport layer implementation when service setup fails.
MulticastReceiver Service for receiving multicast UDP datagrams, one per bound network interface.
MulticastReceiverConfiguration Collection of typically needed configuration settings.
NetworkAddressFactory Configuration utility for network interfaces and addresses.
SOAPActionProcessor Converts UPnP SOAP messages from/to action invocations.
UnsupportedDataException Thrown by processors/converters when errors occured.
UpnpStream A runnable representation of a single HTTP request/response procedure.

Classes in org.teleal.cling.transport.spi used by org.teleal.cling.transport.impl.apache
InitializationException Thrown by the transport layer implementation when service setup fails.
StreamClient Service for sending TCP (HTTP) stream request messages.
StreamClientConfiguration Collection of typically needed configuration settings.
StreamServer Service for receiving TCP (HTTP) streams, one per bound IP address.
StreamServerConfiguration Collection of typically needed configuration settings.
UpnpStream A runnable representation of a single HTTP request/response procedure.

Classes in org.teleal.cling.transport.spi used by org.teleal.cling.transport.spi
DatagramIOConfiguration Collection of typically needed configuration settings.
DatagramProcessor Reads and creates UDP datagrams from and into UPnP messages.
InitializationException Thrown by the transport layer implementation when service setup fails.
MulticastReceiverConfiguration Collection of typically needed configuration settings.
StreamClientConfiguration Collection of typically needed configuration settings.
StreamServerConfiguration Collection of typically needed configuration settings.
UnsupportedDataException Thrown by processors/converters when errors occured.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Copyright © 2011 Teleal GmbH, Switzerland. All Rights Reserved.