Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Interface
org.teleal.cling.transport.spi.MulticastReceiverConfiguration

Packages that use MulticastReceiverConfiguration
org.teleal.cling.transport.impl |
org.teleal.cling.transport.spi |

Uses of MulticastReceiverConfiguration in org.teleal.cling.transport.impl

Classes in org.teleal.cling.transport.impl that implement MulticastReceiverConfiguration
`class` | `MulticastReceiverConfigurationImpl` Settings for the default implementation.

Uses of MulticastReceiverConfiguration in org.teleal.cling.transport.spi

Classes in org.teleal.cling.transport.spi with type parameters of type MulticastReceiverConfiguration
`interface` | `MulticastReceiver<C extends MulticastReceiverConfiguration>` Service for receiving multicast UDP datagrams, one per bound network interface.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Copyright © 2011 Teleal GmbH, Switzerland. All Rights Reserved.