# Cling Core

## User Manual

### Authors:

Christian Bauer

### Table Of Contents:

1. Getting Started

This is how you use Cling:

You need `cling-core.jar` and its dependencies (`seamless-*.jar` files) on your classpath to build and run this code.

2. A first UPnP service and control point

The most basic UPnP service imaginable is the binary light. This device has one service, the power switch, turning the light on and off. In fact, the SwitchPower:1 service and the BinaryLight:1 device are standardized templates you can download here.

In the following sections we'll implement this UPnP service and device with the Cling Core library as a simple Java console application.

2.1. The SwitchPower service implementation

This is the source of the SwitchPower:1 service - note that although there are many annotations in the source, no runtime dependency on Cling exists:

    package example.binarylight;

    import org.fourthline.cling.binding.annotations.*;

    @UpnpService(
            serviceId = @UpnpServiceId("SwitchPower"),
            serviceType = @UpnpServiceType(value = "SwitchPower", version = 1)
    )
    public class SwitchPower {

        @UpnpStateVariable(defaultValue = "0", sendEvents = false)
        private boolean target = false;

        @UpnpStateVariable(defaultValue = "0")
        private boolean status = false;

        @UpnpAction
        public void setTarget(@UpnpInputArgument(name = "NewTargetValue")
                              boolean newTargetValue) {
            target = newTargetValue;
            status = newTargetValue;
            System.out.println("Switch is: " + status);
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "RetTargetValue"))
        public boolean getTarget() {
            return target;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "ResultStatus"))
        public boolean getStatus() {
            // If you want to pass extra UPnP information on error:
            // throw new ActionException(ErrorCode.ACTION_NOT_AUTHORIZED);
            return status;
        }

    }

To compile this class the Cling Core library has to be available on your classpath. However, once compiled this class can be instantiated and executed in any environment, there are no dependencies on any framework or library code.

The annotations are used by Cling to read the metadata that describes your service, what UPnP state variables it has, how they are accessed, and what methods should be exposed as UPnP actions. You can also provide Cling metadata in an XML file or programmatically through Java code - both options are discussed later in this manual. Source code annotations are usually the best choice.

You might have expected something even simpler: After all, a binary light only needs a single boolean state, it is either on or off. The designers of this service also considered that there might be a difference between switching the light on, and actually seeing the result of that action. Imagine what happens if the light bulb is broken: The target state of the light is set to true but the status is still false, because the SetTarget action could not make the switch. Obviously this won't be a problem with this simple demonstration because it only prints the status to standard console output.

2.2. Binding a UPnP device

Devices (and embedded devices) are created programmatically in Cling, with plain Java code that instantiates an immutable graph of objects. The following method creates such a device graph and binds the service from the previous section to the root device:

    LocalDevice createDevice()
            throws ValidationException, LocalServiceBindingException, IOException {

        DeviceIdentity identity =
                new DeviceIdentity(
                        UDN.uniqueSystemIdentifier("Demo Binary Light")
                );

        DeviceType type =
                new UDADeviceType("BinaryLight", 1);

        DeviceDetails details =
                new DeviceDetails(
                        "Friendly Binary Light",
                        new ManufacturerDetails("ACME"),
                        new ModelDetails(
                                "BinLight2000",
                                "A demo light with on/off switch.",
                                "v1"
                        )
                );

        Icon icon =
                new Icon(
                        "image/png", 48, 48, 8,
                        getClass().getResource("icon.png")
                );

        LocalService<SwitchPower> switchPowerService =
                new AnnotationLocalServiceBinder().read(SwitchPower.class);

        switchPowerService.setManager(
                new DefaultServiceManager(switchPowerService, SwitchPower.class)
        );

        return new LocalDevice(identity, type, details, icon, switchPowerService);

        /* Several services can be bound to the same device:
        return new LocalDevice(
                identity, type, details, icon,
                new LocalService[] {switchPowerService, myOtherService}
        );
        */

    }

Let's step through this code. As you can see, all arguments that make up the device's metadata have to be provided through constructors, because the metadata classes are immutable and hence thread-safe.

DeviceIdentity

  Every device, no matter if it is a root device or an embedded device of a root device, requires a unique device name (UDN). This UDN should be stable, that is, it should not change when the device is restarted. When you physically unplug a UPnP appliance from the network (or when you simply turn it off or put it into standby mode), and when you make it available later on, it should expose the same UDN so that clients know they are dealing with the same device. The `UDN.uniqueSystemIdentifier()` method provides exactly that: A unique identifier that is the same every time this method is called on the same computer system. It hashes the network cards hardware address and a few other elements to guarantee uniqueness and stability.

DeviceType

  The type of a device also includes its version, a plain integer. In this case the BinaryLight:1 is a standardized device template which adheres to the UDA (UPnP Device Architecture) specification.

DeviceDetails

  This detailed information about the device's "friendly name", as well as model and manufacturer information is optional. You should at least provide a friendly name value, this is what UPnP applications will display primarily.

Icon

  Every device can have a bunch of icons associated with it which similar to the friendly name are shown to users when appropriate. You do not have to provide any icons if you don't want to, use a constructor of `LocalDevice` without an icon parameter.

Service

  Finally, the most important part of the device are its services. Each `Service` instance encapsulates the metadata for a particular service, what actions and state variables it has, and how it can be invoked. Here we use the Cling annotation binder to instantiate a `Service`, reading the annotation metadata of the `SwitchPower` class.

Because a `Service` instance is only metadata that describes the service, you have to set a `ServiceManager` to do some actual work. This is the link between the metadata and your implementation of a service, where the rubber meets the road. The `DefaultServiceManager` will instantiate the given `SwitchPower` class when an action which operates on the service has to be executed (this happens lazily, as late as possible). The manager will hold on to the instance and always re-use it as long as the service is registered with the UPnP stack. In other words, the service manager is the factory that instantiates your actual implementation of a UPnP service.

Also note that `LocalDevice` is the interface that represents a UPnP device which is "local" to the running UPnP stack on the host. Any device that has been discovered through the network will be a `RemoteDevice` with `RemoteService`'s, you typically do not instantiate these directly.

A `ValidationException` will be thrown when the device graph you instantiated was invaild, you can call `getErrors()` on the exception to find out which property value of which class failed an integrity rule. The local service annotation binder will provide a `LocalServiceBindingException` if something is wrong with your annotation metadata on your service implementation class. An `IOException` can only by thrown by this particular `Icon` constructor, when it reads the resource file.

2.3. Running the server

The Cling Core main API entry point is a thread-safe and typically single shared instance of `UpnpService`:

    package example.binarylight;

    import org.fourthline.cling.UpnpService;
    import org.fourthline.cling.UpnpServiceImpl;
    import org.fourthline.cling.binding.*;
    import org.fourthline.cling.binding.annotations.*;
    import org.fourthline.cling.model.*;
    import org.fourthline.cling.model.meta.*;
    import org.fourthline.cling.model.types.*;

    import java.io.IOException;

    public class BinaryLightServer implements Runnable {

        public static void main(String[] args) throws Exception {
            // Start a user thread that runs the UPnP stack
            Thread serverThread = new Thread(new BinaryLightServer());
            serverThread.setDaemon(false);
            serverThread.start();
        }

        public void run() {
            try {

                final UpnpService upnpService = new UpnpServiceImpl();

                Runtime.getRuntime().addShutdownHook(new Thread() {
                    @Override
                    public void run() {
                        upnpService.shutdown();
                    }
                });

                // Add the bound local device to the registry
                upnpService.getRegistry().addDevice(
                        createDevice()
                );

            } catch (Exception ex) {
                System.err.println("Exception occured: " + ex);
                ex.printStackTrace(System.err);
                System.exit(1);
            }
        }

    }

(The `createDevice()` method from the previous section should be added to this class.)

As soon as the `UPnPServiceImpl` is created, the stack is up and running. You always have to create a `UPnPService` instance, no matter if you write a client or a server. The `UpnpService` maintains a registry of all the discovered remote device on the network, and all the bound local devices. It manages advertisements for discovery and event handling in the background.

You should shut down the UPnP service properly when your application quits, so that all other UPnP systems on your network will be notified that bound devices which are local to your application are no longer available. If you do not shut down the `UpnpService` when your application quits, other UPnP control points on your network might still show devices as available when they are in fact already gone.

The `createDevice()` method from the previous section is called here, as soon as the `Registry` of the local UPnP service stack is available.

You can now compile and start this server, it should print some informational messages to your console and then wait for connections from UPnP control points. Use the Cling Workbench if you want to test your server immediately.

2.4. Creating a control point

The client application has the same basic scaffolding as the server, it also uses a shared single instance of `UpnpService`:

    package example.binarylight;

    import org.fourthline.cling.UpnpService;
    import org.fourthline.cling.UpnpServiceImpl;
    import org.fourthline.cling.controlpoint.*;
    import org.fourthline.cling.model.action.*;
    import org.fourthline.cling.model.message.*;
    import org.fourthline.cling.model.message.header.*;
    import org.fourthline.cling.model.meta.*;
    import org.fourthline.cling.model.types.*;
    import org.fourthline.cling.registry.*;

    public class BinaryLightClient implements Runnable {

        public static void main(String[] args) throws Exception {
            // Start a user thread that runs the UPnP stack
            Thread clientThread = new Thread(new BinaryLightClient());
            clientThread.setDaemon(false);
            clientThread.start();

        }

        public void run() {
            try {

                UpnpService upnpService = new UpnpServiceImpl();

                // Add a listener for device registration events
                upnpService.getRegistry().addListener(
                        createRegistryListener(upnpService)
                );

                // Broadcast a search message for all devices
                upnpService.getControlPoint().search(
                        new STAllHeader()
                );

            } catch (Exception ex) {
                System.err.println("Exception occured: " + ex);
                System.exit(1);
            }
        }

    }

Typically a control point sleeps until a device with a specific type of service becomes available on the network. The `RegistryListener` is called by Cling when a remote device has been discovered - or when it announced itself automatically. Because you usually do not want to wait for the periodic announcements of devices, a control point can also execute a search for all devices (or devices with certain service types or UDN), which will trigger an immediate discovery announcement from those devices that match the search query.

You can already see the `ControlPoint` API here with its `search(...)` method, this is one of the main interfaces you interact with when writing a UPnP client with Cling.

If you compare this code with the server code from the previous section you can see that we are not shutting down the `UpnpService` when the application quits. This is not an issue here, because this application does not have any local devices or service event listeners (not the same as registry listeners) bound and registered. Hence, we do not have to announce their departure on application shutdown and can keep the code simple for the sake of the example.

Let's focus on the registry listener implementation and what happens when a UPnP device has been discovered on the network.

2.5. Executing an action

The control point we are creating here is only interested in services that implement SwitchPower. According to its template definition this service has the `SwitchPower` service identifier, so when a device has been discovered we can check if it offers that service:

    RegistryListener createRegistryListener(final UpnpService upnpService) {
        return new DefaultRegistryListener() {

            ServiceId serviceId = new UDAServiceId("SwitchPower");

            @Override
            public void remoteDeviceAdded(Registry registry, RemoteDevice device) {

                Service switchPower;
                if ((switchPower = device.findService(serviceId)) != null) {

                    System.out.println("Service discovered: " + switchPower);
                    executeAction(upnpService, switchPower);

                }

            }

            @Override
            public void remoteDeviceRemoved(Registry registry, RemoteDevice device) {
                Service switchPower;
                if ((switchPower = device.findService(serviceId)) != null) {
                    System.out.println("Service disappeared: " + switchPower);
                }
            }

        };
    }

If a service becomes available we immediately execute an action on that service. When a `SwitchPower` device disappears from the network a log message is printed. Remember that this is a very trivial control point, it executes a single a fire-and-forget operation when a service becomes available:

    void executeAction(UpnpService upnpService, Service switchPowerService) {

            ActionInvocation setTargetInvocation =
                    new SetTargetActionInvocation(switchPowerService);

            // Executes asynchronous in the background
            upnpService.getControlPoint().execute(
                    new ActionCallback(setTargetInvocation) {

                        @Override
                        public void success(ActionInvocation invocation) {
                            assert invocation.getOutput().length == 0;
                            System.out.println("Successfully called action!");
                        }

                        @Override
                        public void failure(ActionInvocation invocation,
                                            UpnpResponse operation,
                                            String defaultMsg) {
                            System.err.println(defaultMsg);
                        }
                    }
            );

    }

    class SetTargetActionInvocation extends ActionInvocation {

        SetTargetActionInvocation(Service service) {
            super(service.getAction("SetTarget"));
            try {

                // Throws InvalidValueException if the value is of wrong type
                setInput("NewTargetValue", true);

            } catch (InvalidValueException ex) {
                System.err.println(ex.getMessage());
                System.exit(1);
            }
        }
    }

The `Action` (metadata) and the `ActionInvocation` (actual call data) APIs allow very fine-grained control of how an invocation is prepared, how input values are set, how the action is executed, and how the output and outcome is handled. UPnP is inherently asynchronous, so just like the registry listener, executing an action is exposed to you as a callback-style API.

It is recommended that you encapsulate specific action invocations within a subclass of `ActionInvocation`, which gives you an opportunity to further abstract the input and output values of an invocation. Note however that an instance of `ActionInvocation` is not thread-safe and should not be executed in parallel by two threads.

The `ActionCallback` has two main methods you have to implement, one is called when the execution was successful, the other when it failed. There are many reasons why an action execution might fail, read the API documentation for all possible combinations or just print the generated user-friendly default error message.

2.6. Starting the application

Compile the binary light demo application:

Don't forget to copy your `icon.png` file into the `classes` output directory as well, into the right package from which it is loaded as a reasource (the `example.binarylight` package if you followed the previous sections verbatim).

You can start the server or client first, which one doesn't matter as they will discover each other automatically:

You should see discovery and action execution messages on each console. You can stop and restart the applications individually (press CTRL+C on the console).

2.7. Debugging and logging

Although the binary light is a very simple example, you might run into problems. Cling Core helps you resolve most problems with extensive logging. Internally, Cling Core uses Java JDK logging, also known as `java.util.logging` or JUL. There are no wrappers, logging frameworks, logging services, or other dependencies.

By default, the implementation of JUL in the Sun JDK will print only messages with level INFO, WARNING, or SEVERE on `System.out`, and it will print each message over two lines. This is quite inconvenient and ugly, so your first step is probably to configure one line per message. This requires a custom logging handler.

Next you want to configure logging levels for different logging categories. Cling Core will output some INFO level messages on startup and shutdown, but is otherwise silent during runtime unless a problem occurs - it will then log messages at WARNING or SEVERE level.

For debugging, usually more detailed logging levels for various log categories are required. The logging categories in Cling Core are package names, e.g the root logger is available under the name `org.fourthline.cling`. The following tables show typically used categories and the recommended level for debugging:

Network/Transport |
--- | ---
`org.fourthline.cling.transport.spi.DatagramIO (FINE)` `org.fourthline.cling.transport.spi.MulticastReceiver (FINE)` | UDP communication
`org.fourthline.cling.transport.spi.DatagramProcessor (FINER)` | UDP datagram processing and content
`org.fourthline.cling.transport.spi.UpnpStream (FINER)` `org.fourthline.cling.transport.spi.StreamServer (FINE)` `org.fourthline.cling.transport.spi.StreamClient (FINE)` | TCP communication
`org.fourthline.cling.transport.spi.SOAPActionProcessor (FINER)` | SOAP action message processing and content
`org.fourthline.cling.transport.spi.GENAEventProcessor (FINER)` | GENA event message processing and content
`org.fourthline.cling.transport.impl.HttpHeaderConverter (FINER)` | HTTP header processing

UPnP Protocol |
--- | ---
`org.fourthline.cling.protocol.ProtocolFactory (FINER)` `org.fourthline.cling.protocol.async (FINER)` | Discovery (Notification & Search)
`org.fourthline.cling.protocol.ProtocolFactory (FINER)` `org.fourthline.cling.protocol.RetrieveRemoteDescriptors (FINE)` `org.fourthline.cling.protocol.sync.ReceivingRetrieval (FINE)` `org.fourthline.cling.binding.xml.DeviceDescriptorBinder (FINE)` `org.fourthline.cling.binding.xml.ServiceDescriptorBinder (FINE)` | Description
`org.fourthline.cling.protocol.ProtocolFactory (FINER)` `org.fourthline.cling.protocol.sync.ReceivingAction (FINER)` `org.fourthline.cling.protocol.sync.SendingAction (FINER)` | Control
`org.fourthline.cling.model.gena (FINER)` `org.fourthline.cling.protocol.ProtocolFactory (FINER)` `org.fourthline.cling.protocol.sync.ReceivingEvent (FINER)` `org.fourthline.cling.protocol.sync.ReceivingSubscribe (FINER)` `org.fourthline.cling.protocol.sync.ReceivingUnsubscribe (FINER)` `org.fourthline.cling.protocol.sync.SendingEvent (FINER)` `org.fourthline.cling.protocol.sync.SendingSubscribe (FINER)` `org.fourthline.cling.protocol.sync.SendingUnsubscribe (FINER)` `org.fourthline.cling.protocol.sync.SendingRenewal (FINER)` | GENA

Core |
--- | ---
`org.fourthline.cling.transport.Router (FINER)` | Message Router
`org.fourthline.cling.registry.Registry (FINER)` `org.fourthline.cling.registry.LocalItems (FINER)` `org.fourthline.cling.registry.RemoteItems (FINER)` | Registry
`org.fourthline.cling.binding.annotations (FINER)` `org.fourthline.cling.model.meta.LocalService (FINER)` `org.fourthline.cling.model.action (FINER)` `org.fourthline.cling.model.state (FINER)` `org.fourthline.cling.model.DefaultServiceManager (FINER)` | Local service binding & invocation
`org.fourthline.cling.controlpoint (FINER)` | Control Point interaction

One way to configure JUL is with a properties file. For example, create the following file as `mylogging.properties`:

You can now start your application with a system property that names your logging configuration:

You should see the desired log messages printed on `System.out`.

3. The Cling Core API

The programming interface of Cling is fundamentally the same for UPnP clients and servers. The single entry point for any program is the `UpnpService` instance. Through this API you access the local UPnP stack, and either execute operations as a client (control point) or provide services to local or remote clients through the registry.

The following diagram shows the most important interfaces of Cling Core:

You'll be calling these interfaces to work with UPnP devices and interact with UPnP services. Cling provides a fine-grained meta-model representing these artifacts:

In this chapter we'll walk through the API and metamodel in more detail, starting with the `UpnpService`.

3.1. Working with a UpnpService

The `UpnpService` is an interface:

An instance of `UpnpService` represents a running UPnP stack, including all network listeners, background maintenance threads, and so on. Cling Core bundles a default implementation which you can simply instantiate as follows:

With this implementation, the local UPnP stack is ready immediately, it listens on the network for UPnP messages. You should call the `shutdown()` method when you no longer need the UPnP stack. The bundled implementation will then cut all connections with remote event listeners and also notify all other UPnP participants on the network that your local services are no longer available. If you do not shutdown your UPnP stack, remote control points might think that your services are still available until your earlier announcements expire.

The bundled implementation offers two additional constructors:

This constructor accepts your custom `RegistryListener` instances, which will be activated immediately even before the UPnP stack listens on any network interface. This means that you can be notified of all incoming device and service registrations as soon as the network stack is ready. Note that this is rarely useful, you'd typically send search requests after the stack is up and running anyway - after adding listeners to the registry.

The second constructor supports customization of the UPnP stack configuration:

This example configuration will change the TCP listening port of the UPnP stack to `8081`, the default being an ephemeral (system-selected free) port. The `UpnpServiceConfiguration` is also an interface, in the example above you can see how the bundled default implementation is instantiated.

The following section explain the methods of the `UpnpService` interface and what they return in more detail.

3.1.1. Customizing configuration settings

This is the configuration interface of the default UPnP stack in Cling Core, an instance of which you have to provide when creating the `UpnpServiceImpl`:

This is quite an extensive SPI but you typically won't implement it from scratch. Overriding and customizing the bundled `DefaultUpnpServiceConfiguration` should suffice in most cases.

The configuration settings reflect the internal structure of Cling Core:

Network

  The `NetworkAddressFactory` provides the network interfaces, ports, and multicast settings which are used by the UPnP stack. At the time of writing, the following interfaces and IP addresses are ignored by the default configuration: any IPv6 interfaces and addresses, interfaces whose name is "vmnet*", "vnic*", "vboxnet*", "*virtual*", or "ppp*", and the local loopback. Otherwise, all interfaces and their TCP/IP addresses are used and bound.

  You can set the system property `org.fourthline.cling.network.useInterfaces` to provide a comma-separated list of network interfaces you'd like to bind exclusively. Additionally, you can restrict the actual TCP/IP addresses to which the stack will bind with a comma-separated list of IP address provided through the `org.fourthline.cling.network.useAddresses` system property.

  Furthermore, the configuration produces the network-level message receivers and senders, that is, the implementations used by the network `Router`.

  Stream messages are TCP/HTTP requests and responses, the default configuration will use the Sun JDK 6.0 webserver to listen for HTTP requests, and it sends HTTP requests with the standard JDK `HttpURLConnection`. This means there are by default no additional dependencies on any HTTP server/library by Cling Core. However, if you are trying to use Cling Core in a runtime container such as Tomcat, JBoss AS, or Glassfish, you might run into an error on startup. The error tells you that Cling couldn't use the Java JDK's `HTTPURLConnection` for HTTP client operations. This is an old and badly designed part of the JDK: Only "one application" in the whole JVM can configure URL connections. If your container is already using the `HTTPURLConnection`, you have to switch Cling to an alternative HTTP client. See Configuring network transports for other available options and how to change various network-related settings.

  UDP unicast and multicast datagrams are received, parsed, and send by a custom implementation bundled with Cling Core that does not require any particular Sun JDK classes, they should work an all platforms and in any environment.

Processors

  The payload of SSDP datagrams is handled by a default processor, you rarely have to customize it. SOAP action and GENA event messages are also handled by configurable processors, you can provide alternative implementations if necessary, see Switching XML processors. For best interoperability with other (broken) UPnP stacks, consider switching from the strictly specification-compliant default SOAP and GENA processors to the more lenient alternatives.

Descriptors

  Reading and writing UPnP XML device and service descriptors is handled by dedicated binders, see Switching descriptor XML binders. For best interoperability with other (broken) UPnP stacks, consider switching from the strictly specification-compliant default binders to the more lenient alternatives.

Executors

  The Cling UPnP stack is multi-threaded, thread creation and execution is handled through `java.util.concurrent` executors. The default configuration uses a pool of threads with a maximum size of 64 concurrently running threads, which should suffice for even very large installations. Executors can be configured fine-grained, for network message handling, actual UPnP protocol execution (handling discovery, control, and event procedures), and local registry maintenance and listener callback execution. Most likely you will not have to customize any of these settings.

Registry

  Your local device and service XML descriptors and icons can be served with a given `Namespace`, defining how the URL paths of local resources is constructed. You can also configure how frequently Cling will check its `Registry` for outdated devices and expired GENA subscriptions.

There are various other, rarely needed, configuration options available for customizing Cling's behavior, see the Javadoc of `UpnpConfiguration`.

3.1.2. The protocol factory

Cling Core internals are modular and any aspect of the UPnP protocol is handled by an implementation (class) which can be replaced without affecting any other aspect. The `ProtocolFactory` provides implementations, it is always the first access point for the UPnP stack when a message which arrives on the network or an outgoing message has to be handled:

This API is a low-level interface that allows you to access the internals of the UPnP stack, in the rare case you need to manually trigger a particular procedure.

The first two methods are called by the networking code when a message arrives, either multicast or unicast UDP datagrams, or a TCP (HTTP) stream request. The default protocol factory implementation will then pick the appropriate receiving protocol implementation to handle the incoming message.

The local registry of local services known to the UPnP stack naturally also sends messages, such as ALIVE and BYEBYE notifications. Also, if you write a UPnP control point, various search, control, and eventing messages are send by the local UPnP stack. The protocol factory decouples the message sender (registry, control point) from the actual creation, preparation, and transmission of the messages.

Transmission and reception of messages at the lowest-level is the job of the network `Router`.

3.1.3. Accessing low-level network services

The reception and sending of messages, that is, all message transport, is encapsulated through the `Router` interface:

UPnP works with two types of messages: Multicast and unicast UDP datagrams which are typically handled asynchronously, and request/response TCP messages with an HTTP payload. The Cling Core bundled `RouterImpl` will instantiate and maintain the listeners for incoming messages as well as transmit any outgoing messages.

The actual implementation of a message receiver which listens on the network or a message sender is provided by the `UpnpServiceConfiguration`, which we have introduced earlier. You can access the `Router` directly if you have to execute low-level operations on the network layer of the UPnP stack.

Most of the time you will however work with the `ControlPoint` and `Registry` interfaces to interact with the UPnP stack.

3.2. Client operations with ControlPoint

Your primary API when writing a UPnP client application is the `ControlPoint`. An instance is available with `getControlPoint()` on the `UpnpService`.

A UPnP client application typically wants to:

- Search the network for a particular service which it knows how to utilize. Any response to a search request will be delivered asynchronously, so you have to listen to the `Registry` for device registrations, which will occur when devices respond to your search request.
- Execute actions which are offered by services. Action execution is processed asynchronously in Cling Core, and your `ActionCallback` will be notified when the execution was a success (with result values), or a failure (with error status code and messages).
- Subscribe to a service's eventing, so your `SubscriptionCallback` is notified asynchronously when the state of a service changes and an event has been received for your client. You also use the callback to cancel the event subscription when you are no longer interested in state changes.

Let's start with searching for UPnP devices on the network.

3.2.1. Searching the network

When your control point joins the network it probably won't know any UPnP devices and services that might be available. To learn about the present devices it can broadcast - actually with UDP multicast datagrams - a search message which will be received by every device. Each receiver then inspects the search message and decides if it should reply directly (with notification UDP datagrams) to the sending control point.

Search messages carry a search type header and receivers consider this header when they evaluate a potential response. The Cling `ControlPoint` API accepts a `UpnpHeader` argument when creating outgoing search messages.

Most of the time you'd like all devices to respond to your search, this is what the dedicated `STAllHeader` is used for:

    upnpService.getControlPoint().search(
            new STAllHeader()
    );

Notification messages will be received by your control point and you can listen to the `Registry` and inspect the found devices and their services. (By the way, if you call `search()` without any argument, that's the same.)

On the other hand, when you already know the unique device name (UDN) of the device you are searching for - maybe because your control point remembered it while it was turned off - you can send a message which will trigger a response from only a particular device:

    upnpService.getControlPoint().search(
            new UDNHeader(udn)
    );

This is mostly useful to avoid network congestion when dozens of devices might all respond to a search request. Your `Registry` listener code however still has to inspect each newly found device, as registrations might occur independently from searches.

You can also search by device or service type. This search request will trigger responses from all devices of type "`urn:schemas-upnp-org:device:BinaryLight:1`":

    UDADeviceType udaType = new UDADeviceType("BinaryLight");
    upnpService.getControlPoint().search(
            new UDADeviceTypeHeader(udaType)
    );

If the desired device type is of a custom namespace, use this variation:

    DeviceType type = new DeviceType("org-mydomain", "MyDeviceType", 1);
    upnpService.getControlPoint().search(
            new DeviceTypeHeader(type)
    );

Or, you can search for all devices which implement a particular service type:

    UDAServiceType udaType = new UDAServiceType("SwitchPower");
    upnpService.getControlPoint().search(
            new UDAServiceTypeHeader(udaType)
    );

    ServiceType type = new ServiceType("org-mydomain", "MyServiceType", 1);
    upnpService.getControlPoint().search(
            new ServiceTypeHeader(type)
    );

3.2.2. Invoking an action

UPnP services expose state variables and actions. While the state variables represent the current state of the service, actions are the operations used to query or maniuplate the service's state. You have to obtain a `Service` instance from a `Device` to access any `Action`. The target device can be local to the same UPnP stack as your control point, or it can be remote of another device anywhere on the network. We'll discuss later in this chapter how to access devices through the local stack's `Registry`.

Once you have the device, access the `Service` through the metadata model, for example:

    Service service = device.findService(new UDAServiceId("SwitchPower"));
    Action getStatusAction = service.getAction("GetStatus");

This method will search the device and all its embedded devices for a service with the given identifier and returns either the found `Service` or `null`. The Cling metamodel is thread-safe, so you can share an instance of `Service` or `Action` and access it concurrently.

Invoking an action is the job of an instance of `ActionInvocation`, note that this instance is NOT thread-safe and each thread that wishes to execute an action has to obtain its own invocation from the `Action` metamodel:

    ActionInvocation getStatusInvocation = new ActionInvocation(getStatusAction);

    ActionCallback getStatusCallback = new ActionCallback(getStatusInvocation) {

        @Override
        public void success(ActionInvocation invocation) {
            ActionArgumentValue status  = invocation.getOutput("ResultStatus");

            assert status != null;

            assertEquals(status.getArgument().getName(), "ResultStatus");

            assertEquals(status.getDatatype().getClass(), BooleanDatatype.class);
            assertEquals(status.getDatatype().getBuiltin(), Datatype.Builtin.BOOLEAN);

            assertEquals((Boolean) status.getValue(), Boolean.valueOf(false));
            assertEquals(status.toString(), "0"); // '0' is 'false' in UPnP
        }

        @Override
        public void failure(ActionInvocation invocation,
                            UpnpResponse operation,
                            String defaultMsg) {
            System.err.println(defaultMsg);
        }
    };

    upnpService.getControlPoint().execute(getStatusCallback);

Execution is asynchronous, your `ActionCallback` has two methods which will be called by the UPnP stack when the execution completes. If the action is successful, you can obtain any output argument values from the invocation instance, which is conveniently passed into the `success()` method. You can inspect the named output argument values and their datatypes to continue processing the result.

Action execution doesn't have to be processed asynchronously, after all, the underlying HTTP/SOAP protocol is a request waiting for a response. The callback programming model however fits nicely into a typical UPnP client, which also has to process event notifications and device registrations asynchronously. If you want to execute an `ActionInvocation` directly, within the current thread, use the empty `ActionCallback.Default` implementation:

    new ActionCallback.Default(getStatusInvocation, upnpService.getControlPoint()).run();

When invocation fails you can access the failure details through `invocation.getFailure()`, or use the shown convenience method to create a simple error message. See the Javadoc of `ActionCallback` for more details.

When an action requires input argument values, you have to provide them. Like output arguments, any input arguments of actions are also named, so you can set them by calling `setInput("MyArgumentName", value)`:

    Action action = service.getAction("SetTarget");

    ActionInvocation setTargetInvocation = new ActionInvocation(action);

    setTargetInvocation.setInput("NewTargetValue", true); // Can throw InvalidValueException

    // Alternative:
    //
    // setTargetInvocation.setInput(
    //         new ActionArgumentValue(
    //                 action.getInputArgument("NewTargetValue"),
    //                 true
    //         )
    // );

    ActionCallback setTargetCallback = new ActionCallback(setTargetInvocation) {

        @Override
        public void success(ActionInvocation invocation) {
            ActionArgumentValue[] output = invocation.getOutput();
            assertEquals(output.length, 0);
        }

        @Override
        public void failure(ActionInvocation invocation,
                            UpnpResponse operation,
                            String defaultMsg) {
            System.err.println(defaultMsg);
        }
    };

    upnpService.getControlPoint().execute(setTargetCallback);

This action has one input argument of UPnP type "boolean". You can set a Java `boolean` primitive or `Boolean` instance and it will be automatically converted. If you set an invalid value for a particular argument, such as an instance with the wrong type, an `InvalidValueException` will be thrown immediately.

Empty values and null in Cling
There is no difference between empty string `""` and `null` in Cling, because the UPnP specification does not address this issue. The SOAP message of an action call or an event message must contain an element `` for all arguments, even if it is an empty XML element. If you provide an empty string or a null value when preparing a message, it will always be a `null` on the receiving end because we can only transmit one thing, an empty XML element. If you forget to set an input argument's value, it will be null/empty element.
3.2.3. Receiving events from services

The UPnP specification defines a general event notification architecture (GENA) which is based on a publish/subscribe paradigm. Your control point subscribes with a service in order to receive events. When the service state changes, an event message will be delivered to the callback of your control point. Subscriptions are periodically refreshed until you unsubscribe from the service. If you do not unsubscribe and if a refresh of the subscription fails, maybe because the control point was turned off without proper shutdown, the subscription will timeout on the publishing service's side.

This is an example subscription on a service that sends events for a state variable named `Status` (e.g. the previously shown SwitchPower service). The subscription's refresh and timeout period is 600 seconds:

    SubscriptionCallback callback = new SubscriptionCallback(service, 600) {

        @Override
        public void established(GENASubscription sub) {
            System.out.println("Established: " + sub.getSubscriptionId());
        }

        @Override
        protected void failed(GENASubscription subscription,
                              UpnpResponse responseStatus,
                              Exception exception,
                              String defaultMsg) {
            System.err.println(defaultMsg);
        }

        @Override
        public void ended(GENASubscription sub,
                          CancelReason reason,
                          UpnpResponse response) {
            assertNull(reason);
        }

        @Override
        public void eventReceived(GENASubscription sub) {

            System.out.println("Event: " + sub.getCurrentSequence().getValue());

            Map<String, StateVariableValue> values = sub.getCurrentValues();
            StateVariableValue status = values.get("Status");

            assertEquals(status.getDatatype().getClass(), BooleanDatatype.class);
            assertEquals(status.getDatatype().getBuiltin(), Datatype.Builtin.BOOLEAN);

            System.out.println("Status is: " + status.toString());

        }

        @Override
        public void eventsMissed(GENASubscription sub, int numberOfMissedEvents) {
            System.out.println("Missed events: " + numberOfMissedEvents);
        }

        @Override
        protected void invalidMessage(RemoteGENASubscription sub,
                                      UnsupportedDataException ex) {
            // Log/send an error report?
        }
    };

    upnpService.getControlPoint().execute(callback);

The `SubscriptionCallback` offers the methods `failed()`, `established()`, and `ended()` which are called during a subscription's lifecycle. When a subscription ends you will be notified with a `CancelReason` whenever the termination of the subscription was irregular. See the Javadoc of these methods for more details.

Every event message from the service will be passed to the `eventReceived()` method, and every message will carry a sequence number. You can access the changed state variable values in this method, note that only state variables which changed are included in the event messages. A special event message called the "initial event" will be send by the service once, when you subscribe. This message contains values for all evented state variables of the service; you'll receive an initial snapshot of the state of the service at subscription time.

Whenever the receiving UPnP stack detects an event message that is out of sequence, e.g. because some messages were lost during transport, the `eventsMissed()` method will be called before you receive the event. You then decide if missing events is important for the correct behavior of your application, or if you can silently ignore it and continue processing events with non-consecutive sequence numbers.

You can optionally override the `invalidMessage()` method and react to message parsing errors, if your subscription is with a remote service. Most of the time all you can do here is log or report an error to developers, so they can work around the broken remote service (UPnP interoperability is frequently very poor).

You end a subscription regularly by calling `callback.end()`, which will unsubscribe your control point from the service.

3.3. The Registry

The `Registry`, which you access with `getRegistry()` on the `UpnpService`, is the heart of a Cling Core UPnP stack. The registry is responsible for:

- Maintaining discovered UPnP devices on your network. It also offers a management API so you can register local devices and offer local services. This is how you expose your own UPnP devices on the network. The registry handles all notification, expiration, request routing, refreshing, and so on.
- Managing GENA (general event & notification architecture) subscriptions. Any outgoing subscription to a remote service is known by the registry, it is refreshed periodically so it doesn't expire. Any incoming eventing subscription to a local service is also known and maintained by the registry (expired and removed when necessary).
- Providing the interface for the addition and removal of `RegistryListener` instances. A registry listener is used in client or server UPnP applications, it provides a uniform interface for notification of registry events. Typically, you write and register a listener to be notified when a service you want to work with becomes available on the network - on a local or remote device - and when it disappears.

3.3.1. Browsing the Registry

Although you typically create a `RegistryListener` to be notified of discovered and disappearing UPnP devices on your network, sometimes you have to browse the `Registry` manually.

The following call will return a device with the given unique device name, but only a root device and not any embedded device. Set the second parameter of `registry.getDevice()` to `false` if the device you are looking for might be an embedded device.

    Registry registry = upnpService.getRegistry();
    Device foundDevice = registry.getDevice(udn, true);

    assertEquals(foundDevice.getIdentity().getUdn(), udn);

If you know that the device you need is a `LocalDevice` - or a `RemoteDevice` - you can use the following operation:

    LocalDevice localDevice = registry.getLocalDevice(udn, true);

Most of the time you need a device that is of a particular type or that implements a particular service type, because this is what your control point can handle:

    DeviceType deviceType = new UDADeviceType("MY-DEVICE-TYPE", 1);
    Collection<Device> devices = registry.getDevices(deviceType);

    ServiceType serviceType = new UDAServiceType("MY-SERVICE-TYPE-ONE", 1);
    Collection<Device> devices = registry.getDevices(serviceType);

3.3.2. Listening to registry changes

The `RegistryListener` is your primary API when discovering devices and services with your control point. UPnP operates asynchronous, so advertisements (either alive or byebye) of devices can occur at any time. Responses to your network search messages are also asynchronous.

This is the interface:

    public interface RegistryListener {

        public void remoteDeviceDiscoveryStarted(Registry registry, RemoteDevice device);

        public void remoteDeviceDiscoveryFailed(Registry registry, RemoteDevice device, Exception ex);

        public void remoteDeviceAdded(Registry registry, RemoteDevice device);

        public void remoteDeviceUpdated(Registry registry, RemoteDevice device);

        public void remoteDeviceRemoved(Registry registry, RemoteDevice device);

        public void localDeviceAdded(Registry registry, LocalDevice device);

        public void localDeviceRemoved(Registry registry, LocalDevice device);

    }

Typically you don't want to implement all of these methods. Some are only useful if you write a service or a generic control point. Most of the time you want to be notified when a particular device with a particular service appears on your network. So it is much easier to extend the `DefaultRegistryListener`, which has empty implementations for all methods of the interface, and only override the methods you need.

The `remoteDeviceDiscoveryStarted()` and `remoteDeviceDiscoveryFailed()` methods are completely optional but useful on slow machines (such as Android handsets). Cling will retrieve and initialize all device metadata for each UPnP device before it will announce it on the `Registry`. UPnP metadata is split into several XML descriptors, so retrieval via HTTP of these descriptors, parsing, and validating all metadata for a complex UPnP device and service model can take several seconds. These two methods allow you to access the device as soon as possible, after the first descriptor has been retrieved and parsed. At this time the services metadata is however not available:

    public class QuickstartRegistryListener extends DefaultRegistryListener {

        @Override
        public void remoteDeviceDiscoveryStarted(Registry registry, RemoteDevice device) {

            // You can already use the device here and you can see which services it will have
            assertEquals(device.findServices().length, 3);

            // But you can't use the services
            for (RemoteService service : device.findServices()) {
                assertEquals(service.getActions().length, 0);
                assertEquals(service.getStateVariables().length, 0);
            }
        }

        @Override
        public void remoteDeviceDiscoveryFailed(Registry registry, RemoteDevice device, Exception ex) {
            // You might want to drop the device, its services couldn't be hydrated
        }
    }

This is how you register and activate a listener:

    QuickstartRegistryListener listener = new QuickstartRegistryListener();
    upnpService.getRegistry().addListener(listener);

Most of the time, on any device that is faster than a cellphone, your listeners will look like this:

    public class MyListener extends DefaultRegistryListener {

        @Override
        public void remoteDeviceAdded(Registry registry, RemoteDevice device) {
            Service myService = device.findService(new UDAServiceId("MY-SERVICE-123"));
            if (myService != null) {
                // Do something with the discovered service
            }
        }

        @Override
        public void remoteDeviceRemoved(Registry registry, RemoteDevice device) {
            // Stop using the service if this is the same device, it's gone now
        }
    }

The device metadata of the parameter to `remoteDeviceAdded()` is fully hydrated, all of its services, actions, and state variables are available. You can continue with this metadata, writing action invocations and event monitoring callbacks. You also might want to react accordingly when the device disappears from the network.

4. Creating and binding services

Out of the box, any Java class can be a UPnP service. Let's go back to the first example of a UPnP service in chapter 1, the SwitchPower:1 service implementation, repeated here:

    package example.binarylight;

    import org.fourthline.cling.binding.annotations.*;

    @UpnpService(
            serviceId = @UpnpServiceId("SwitchPower"),
            serviceType = @UpnpServiceType(value = "SwitchPower", version = 1)
    )
    public class SwitchPower {

        @UpnpStateVariable(defaultValue = "0", sendEvents = false)
        private boolean target = false;

        @UpnpStateVariable(defaultValue = "0")
        private boolean status = false;

        @UpnpAction
        public void setTarget(@UpnpInputArgument(name = "NewTargetValue")
                              boolean newTargetValue) {
            target = newTargetValue;
            status = newTargetValue;
            System.out.println("Switch is: " + status);
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "RetTargetValue"))
        public boolean getTarget() {
            return target;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "ResultStatus"))
        public boolean getStatus() {
            // If you want to pass extra UPnP information on error:
            // throw new ActionException(ErrorCode.ACTION_NOT_AUTHORIZED);
            return status;
        }

    }

This class depends on the `org.fourthline.cling.annotation` package at compile-time. The metadata encoded in these source annotations is preserved in the bytecode and Cling will read it at runtime when you bind the service ("binding" is just a fancy word for reading and writing metadata). You can load and execute this class without accessing the annotations, in any environment and without having the Cling libraries on your classpath. This is a compile-time dependency only.

Cling annotations give you much flexibility in designing your service implementation class, as shown in the following examples.

4.1. Annotating a service implementation

The previously shown service class had a few annotations on the class itself, declaring the name and version of the service. Then annotations on fields were used to declare the state variables of the service and annotations on methods to declare callable actions.

Your service implementation might not have fields that directly map to UPnP state variables.

4.1.1. Mapping state variables

The following example only has a single field named `power`, however, the UPnP service requires two state variables. In this case you declare the UPnP state variables with annotations on the class:

    @UpnpService(
            serviceId = @UpnpServiceId("SwitchPower"),
            serviceType = @UpnpServiceType(value = "SwitchPower", version = 1)

    )
    @UpnpStateVariables(
            {
                    @UpnpStateVariable(
                            name = "Target",
                            defaultValue = "0",
                            sendEvents = false
                    ),
                    @UpnpStateVariable(
                            name = "Status",
                            defaultValue = "0"
                    )
            }
    )
    public class SwitchPowerAnnotatedClass {

        private boolean power;

        @UpnpAction
        public void setTarget(@UpnpInputArgument(name = "NewTargetValue")
                              boolean newTargetValue) {
            power = newTargetValue;
            System.out.println("Switch is: " + power);
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "RetTargetValue"))
        public boolean getTarget() {
            return power;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "ResultStatus"))
        public boolean getStatus() {
            return power;
        }
    }

The `power` field is not mapped to the state variables and you are free to design your service internals as you like. Did you notice that you never declared the datatype of your state variables? Also, how can Cling read the "current state" of your service for GENA subscribers or when a "query state variable" action is received? Both questions have the same answer.

Let's consider GENA eventing first. This example has an evented state variable called `Status`, and if a control point subscribes to the service to be notified of changes, how will Cling obtain the current status? If you'd have used `@UpnpStateVariable` on your fields, Cling would then directly access field values through Java Reflection. On the other hand if you declare state variables not on fields but on your service class, Cling will during binding detect any JavaBean-style getter method that matches the derived property name of the state variable.

In other words, Cling will discover that your class has a `getStatus()` method. It doesn't matter if that method is also an action-mapped method, the important thing is that it matches JavaBean property naming conventions. The `Status` UPnP state variable maps to the `status` property, which is expected to have a `getStatus()` accessor method. Cling will use this method to read the current state of your service for GENA subscribers and when the state variable is manually queried.

If you do not provide a UPnP datatype name in your `@UpnpStateVariable` annotation, Cling will use the type of the annotated field or discovered JavaBean getter method to figure out the type. The supported default mappings between Java types and UPnP datatypes are shown in the following table:

Java Type | UPnP Datatype
--- | ---
`java.lang.Boolean` | `boolean`
`boolean` | `boolean`
`java.lang.Short` | `i2`
`short` | `i2`
`java.lang.Integer` | `i4`
`int` | `i4`
`org.fourthline.cling.model.types.UnsignedIntegerOneByte` | `ui1`
`org.fourthline.cling.model.types.UnsignedIntegerTwoBytes` | `ui2`
`org.fourthline.cling.model.types.UnsignedIntegerFourBytes` | `ui4`
`java.lang.Float` | `r4`
`float` | `r4`
`java.lang.Double` | `float`
`double` | `float`
`java.lang.Character` | `char`
`char` | `char`
`java.lang.String` | `string`
`java.util.Calendar` | `datetime`
`byte[]` | `bin.base64`
`java.net.URI` | `uri`

Cling tries to provide smart defaults. For example, the previously shown service classes did not name the related state variable of action output arguments, as required by UPnP. Cling will automatically detect that the `getStatus()` method is a JavaBean getter method (its name starts with `get` or `is`) and use the JavaBean property name to find the related state variable. In this case that would be the JavaBean property `status` and Cling is also smart enough to know that you really want the uppercase UPnP state variable named `Status`.

4.1.2. Explicitly naming related state variables

If your mapped action method does not match the name of a mapped state variable, you have to provide the name of (any) argument's related state variable:

    @UpnpAction(
            name = "GetStatus",
            out = @UpnpOutputArgument(
                    name = "ResultStatus",
                    stateVariable = "Status"
            )
    )
    public boolean retrieveStatus() {
        return status;
    }

Here the method has the name `retrieveStatus`, which you also have to override if you want it be known as a the `GetStatus` UPnP action. Because it is no longer a JavaBean accessor for `status`, it explicitly has to be linked with the related state variable `Status`. You always have to provide the related state variable name if your action has more than one output argument.

The "related statevariable" detection algorithm in Cling has one more trick up its sleeve however. The UPnP specification says that a state variable which is only ever used to describe the type of an input or output argument should be named with the prefix `A_ARG_TYPE_`. So if you do not name the related state variable of your action argument, Cling will also look for a state variable with the name `A_ARG_TYPE_[Name Of Your Argument]`. In the example above, Cling is therefore also searching (unsuccessfully) for a state variable named `A_ARG_TYPE_ResultStatus`. (Given that direct querying of state variables is already deprecated in UDA 1.0, there are NO state variables which are anything but type declarations for action input/output arguments. This is a good example why UPnP is such a horrid specification.)

For the next example, let's assume you have a class that was already written, not necessarily as a service backend for UPnP but for some other purpose. You can't redesign and rewrite your class without interrupting all existing code. Cling offers some flexibility in the mapping of action methods, especially how the output of an action call is obtained.

4.1.3. Getting an output value from another method

In the following example, the UPnP action has an output argument but the mapped method is void and does not return any value:

    public boolean getStatus() {
        return status;
    }

    @UpnpAction(
            name = "GetStatus",
            out = @UpnpOutputArgument(
                    name = "ResultStatus",
                    getterName = "getStatus"
            )
    )
    public void retrieveStatus() {
        // NOOP in this example
    }

By providing a `getterName` in the annotation you can instruct Cling to call this getter method when the action method completes, taking the getter method's return value as the output argument value. If there are several output arguments you can map each to a different getter method.

Alternatively, and especially if an action has several output arguments, you can return multiple values wrapped in a JavaBean from your action method.

4.1.4. Getting output values from a JavaBean

Here the action method does not return the output argument value directly, but a JavaBean instance is returned which offers a getter method to obtain the output argument value:

    @UpnpAction(
            name = "GetStatus",
            out = @UpnpOutputArgument(
                    name = "ResultStatus",
                    getterName = "getWrapped"
            )
    )
    public StatusHolder getStatus() {
        return new StatusHolder(status);
    }

    public class StatusHolder {
        boolean wrapped;

        public StatusHolder(boolean wrapped) {
            this.wrapped = wrapped;
        }

        public boolean getWrapped() {
            return wrapped;
        }
    }

Cling will detect that you mapped a getter name in the output argument and that the action method is not `void`. It now expects that it will find the getter method on the returned JavaBean. If there are several output arguments, all of them have to be mapped to getter methods on the returned JavaBean.

An important piece is missing from the SwitchPower:1 implementation: It doesn't fire any events when the status of the power switch changes. This is in fact required by the specification that defines the SwitchPower:1 service. The following section explains how you can propagate state changes from within your UPnP service to local and remote subscribers.

4.2. Providing events on service state changes

The standard mechanism in the JDK for eventing is the `PropertyChangeListener` reacting on a `PropertyChangeEvent`. Cling utilizes this API for service eventing, thus avoiding a dependency between your service code and proprietary APIs.

Consider the following modification of the original SwitchPower:1 implementation:

    package example.localservice;

    import org.fourthline.cling.binding.annotations.*;
    import java.beans.PropertyChangeSupport;

    @UpnpService(
            serviceId = @UpnpServiceId("SwitchPower"),
            serviceType = @UpnpServiceType(value = "SwitchPower", version = 1)
    )
    public class SwitchPowerWithPropertyChangeSupport {

        private final PropertyChangeSupport propertyChangeSupport;

        public SwitchPowerWithPropertyChangeSupport() {
            this.propertyChangeSupport = new PropertyChangeSupport(this);
        }

        public PropertyChangeSupport getPropertyChangeSupport() {
            return propertyChangeSupport;
        }

        @UpnpStateVariable(defaultValue = "0", sendEvents = false)
        private boolean target = false;

        @UpnpStateVariable(defaultValue = "0")
        private boolean status = false;

        @UpnpAction
        public void setTarget(@UpnpInputArgument(name = "NewTargetValue") boolean newTargetValue) {

            boolean targetOldValue = target;
            target = newTargetValue;
            boolean statusOldValue = status;
            status = newTargetValue;

            // These have no effect on the UPnP monitoring but it's JavaBean compliant
            getPropertyChangeSupport().firePropertyChange("target", targetOldValue, target);
            getPropertyChangeSupport().firePropertyChange("status", statusOldValue, status);

            // This will send a UPnP event, it's the name of a state variable that triggers events
            getPropertyChangeSupport().firePropertyChange("Status", statusOldValue, status);
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "RetTargetValue"))
        public boolean getTarget() {
            return target;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "ResultStatus"))
        public boolean getStatus() {
            return status;
        }

    }

The only additional dependency is on `java.beans.PropertyChangeSupport`. Cling detects the `getPropertyChangeSupport()` method of your service class and automatically binds the service management on it. You will have to have this method for eventing to work with Cling. You can create the `PropertyChangeSupport` instance in your service's constructor or any other way, the only thing Cling is interested in are property change events with the "property" name of a UPnP state variable.

Consequently, `firePropertyChange("NameOfAStateVariable")` is how you tell Cling that a state variable value has changed. It doesn't even matter if you call `firePropertyChange("Status", null, null)` or `firePropertyChange("Status", oldValue, newValue)`. Cling only cares about the state variable name; it will then check if the state variable is evented and pull the data out of your service implementation instance by accessing the appropriate field or a getter. Any "old" or "new" value you pass along is ignored.

Also note that `firePropertyChange("Target", null, null)` would have no effect, because `Target` is mapped with `sendEvents="false"`.

Most of the time a JavaBean property name is not the same as UPnP state variable name. For example, the JavaBean `status` property name is lowercase, while the UPnP state variable name is uppercase `Status`. The Cling eventing system ignores any property change event that doesn't exactly name a service state variable. This allows you to use JavaBean eventing independently from UPnP eventing, e.g. for GUI binding (Swing components also use the JavaBean eventing system).

Let's assume for the sake of the next example that `Target` actually is also evented, like `Status`. If several evented state variables change in your service, but you don't want to trigger individual change events for each variable, you can combine them in a single event as a comma-separated list of state variable names:

    @UpnpAction
    public void setTarget(@UpnpInputArgument(name = "NewTargetValue") boolean newTargetValue) {

        target = newTargetValue;
        status = newTargetValue;

        // If several evented variables changed, bundle them in one event separated with commas:
        getPropertyChangeSupport().firePropertyChange(
            "Target, Status", null, null
        );

        // Or if you don't like string manipulation:
        // getPropertyChangeSupport().firePropertyChange(
        //    ModelUtil.toCommaSeparatedList(new String[]{"Target", "Status"}), null, null
        //);
    }

More advanced mappings are possible and often required, as shown in the next examples. We are now leaving the SwitchPower service behind, as it is no longer complex enough.

4.3. Converting string action argument values

The UPnP specification defines no framework for custom datatypes. The predictable result is that service designers and vendors are overloading strings with whatever semantics they consider necessary for their particular needs. For example, the UPnP A/V specifications often require lists of values (like a list of strings or a list of numbers), which are then transported between service and control point as a single string - the individual values are represented in this string separated by commas.

Cling supports these conversions and it tries to be as transparent as possible.

4.3.1. String value converters

Consider the following service class with all state variables of `string` UPnP datatype - but with a much more specific Java type:

    import org.fourthline.cling.model.types.csv.CSV;
    import org.fourthline.cling.model.types.csv.CSVInteger;

    @UpnpService(
            serviceId = @UpnpServiceId("MyService"),
            serviceType = @UpnpServiceType(namespace = "mydomain", value = "MyService"),
            stringConvertibleTypes = MyStringConvertible.class
    )
    public class MyServiceWithStringConvertibles {

        @UpnpStateVariable
        private URL myURL;

        @UpnpStateVariable
        private URI myURI;

        @UpnpStateVariable(datatype = "string")
        private List<Integer> myNumbers;

        @UpnpStateVariable
        private MyStringConvertible myStringConvertible;

        @UpnpAction(out = @UpnpOutputArgument(name = "Out"))
        public URL getMyURL() {
            return myURL;
        }

        @UpnpAction
        public void setMyURL(@UpnpInputArgument(name = "In") URL myURL) {
            this.myURL = myURL;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "Out"))
        public URI getMyURI() {
            return myURI;
        }

        @UpnpAction
        public void setMyURI(@UpnpInputArgument(name = "In") URI myURI) {
            this.myURI = myURI;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "Out"))
        public CSV<Integer> getMyNumbers() {
            CSVInteger wrapper = new CSVInteger();
            if (myNumbers != null)
                wrapper.addAll(myNumbers);
            return wrapper;
        }

        @UpnpAction
        public void setMyNumbers(
                @UpnpInputArgument(name = "In")
                CSVInteger myNumbers
        ) {
            this.myNumbers = myNumbers;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "Out"))
        public MyStringConvertible getMyStringConvertible() {
            return myStringConvertible;
        }

        @UpnpAction
        public void setMyStringConvertible(
                @UpnpInputArgument(name = "In")
                MyStringConvertible myStringConvertible
        ) {
            this.myStringConvertible = myStringConvertible;
        }
    }

The state variables are all of UPnP datatype `string` because Cling knows that the Java type of the annotated field is "string convertible". This is always the case for `java.net.URI` and `java.net.URL`.

Any other Java type you'd like to use for automatic string conversion has to be named in the `@UpnpService` annotation on the class, like the `MyStringConvertible`. Note that these types have to have an appropriate `toString()` method and a single argument constructor that accepts a `java.lang.String` ("from string" conversion).

The `List<Integer>` is the collection you'd use in your service implementation to group several numbers. Let's assume that for UPnP communication you need a comma-separated representation of the individual values in a string, as is required by many of the UPnP A/V specifications. First, tell Cling that the state variable really is a string datatype, it can't infer that from the field type. Then, if an action has this output argument, instead of manually creating the comma-separated string you pick the appropriate converter from the classes in `org.fourthline.cling.model.types.csv.*` and return it from your action method. These are actually `java.util.List` implementations, so you could use them instead of `java.util.List` if you don't care about the dependency. Any action input argument value can also be converted from a comma-separated string representation to a list automatically - all you have to do is use the CSV converter class as an input argument type.

4.3.2. Working with enums

Java `enum`'s are special, unfortunately: Cling can convert your enum value into a string for transport in UPnP messages, but you have to convert it back manually from a string. This is shown in the following service example:

    @UpnpService(
            serviceId = @UpnpServiceId("MyService"),
            serviceType = @UpnpServiceType(namespace = "mydomain", value = "MyService"),
            stringConvertibleTypes = MyStringConvertible.class
    )
    public class MyServiceWithEnum {

        public enum Color {
            Red,
            Green,
            Blue
        }

        @UpnpStateVariable
        private Color color;

        @UpnpAction(out = @UpnpOutputArgument(name = "Out"))
        public Color getColor() {
            return color;
        }

        @UpnpAction
        public void setColor(@UpnpInputArgument(name = "In") String color) {
            this.color = Color.valueOf(color);
        }

    }

Cling will automatically assume that the datatype is a UPnP string if the field (or getter) or getter Java type is an enum. Furthermore, an `<allowedValueList>` will be created in your service descriptor XML, so control points know that this state variable has in fact a defined set of possible values.

4.4. Restricting allowed state variable values

The UPnP specification defines a set of rules for restricting legal values of state variables, in addition to their type. For string-typed state variables, you can provide a list of exclusively allowed strings. For numeric state variables, a value range with minimum, maximum, and allowed "step" (the interval) can be provided.

4.4.1. Exclusive list of string values

If you have a static list of legal string values, set it directly on the annotation of your state variable's field:

    @UpnpStateVariable(
        allowedValues = {"Foo", "Bar", "Baz"}
    )
    private String restricted;

Alternatively, if your allowed values have to be determined dynamically when your service is being bound, you can implement a class with the `org.fourthline.cling.binding.AllowedValueProvider` interface:

    public static class MyAllowedValueProvider implements AllowedValueProvider {
        @Override
        public String[] getValues() {
            return new String[] {"Foo", "Bar", "Baz"};
        }
    }

Then, instead of specifying a static list of string values in your state variable declaration, name the provider class:

    @UpnpStateVariable(
        allowedValueProvider= MyAllowedValueProvider.class
    )
    private String restricted;

Note that this provider will only be queried when your annotations are being processed, once when your service is bound in Cling.

4.4.2. Restricting numeric value ranges

For numeric state variables, you can limit the set of legal values within a range when declaring the state variable:

    @UpnpStateVariable(
        allowedValueMinimum = 10,
        allowedValueMaximum = 100,
        allowedValueStep = 5
    )
    private int restricted;

Alternatively, if your allowed range has to be determined dynamically when your service is being bound, you can implement a class with the `org.fourthline.cling.binding.AllowedValueRangeProvider` interface:

    public static class MyAllowedValueProvider implements AllowedValueRangeProvider {
        @Override
        public long getMinimum() {
            return 10;
        }

        @Override
        public long getMaximum() {
            return 100;
        }

        @Override
        public long getStep() {
            return 5;
        }
    }

Then, instead of specifying a static list of string values in your state variable declaration, name the provider class:

    @UpnpStateVariable(
        allowedValueRangeProvider = MyAllowedValueProvider.class
    )
    private int restricted;

Note that this provider will only be queried when your annotations are being processed, once when your service is bound in Cling.

5. Cling on Android

Cling Core provides a UPnP stack for Android applications. Typically you'd write control point applications, as most Android systems today are small hand-held devices. You can however also write UPnP server applications on Android, all features of Cling Core are supported.

Android platform level 15 (4.0) is required for Cling 2.x, use Cling 1.x to support older Android versions.

Cling on the Android emulator
At the time of writing, receiving UDP Multicast datagrams was not supported by the Android emulator. The emulator will send (multicast) UDP datagrams, however. You will be able to send a multicast UPnP search and receive UDP unicast responses, therefore discover existing running devices. You will not discover devices which have been turned on after your search, and you will not receive any message when a device is switched off. Other control points on your network will not discover your local Android device/services at all. All of this can be confusing when testing your application, so unless you really understand what works and what doesn't, you might want to use a real device instead.

The following examples are based on the Cling demo applications for Android, the `cling-demo-android-browser` and the `cling-demo-android-light`, available in the Cling distribution.

5.1. Configuring the application service

You could instantiate the Cling `UpnpService` as usual in your Android application's main activity. On the other hand, if several activities in your application require access to the UPnP stack, a better design would utilize a background `android.app.Service`. Any activity that wants to access the UPnP stack can then bind and unbind from this service as needed.

The interface of such a service component is available in Cling as `org.fourthline.cling.android.AndroidUpnpService`:

    public interface AndroidUpnpService {

        /**
         * @return The actual main instance and interface of the UPnP service.
         */
        public UpnpService get();

        /**
         * @return The configuration of the UPnP service.
         */
        public UpnpServiceConfiguration getConfiguration();

        /**
         * @return The registry of the UPnP service.
         */
        public Registry getRegistry();

        /**
         * @return The client API of the UPnP service.
         */
        public ControlPoint getControlPoint();

    }

An activity typically accesses the `Registry` of known UPnP devices or searches for and controls UPnP devices with the `ControlPoint`.

You have to configure the built-in implementation of this service component in your `AndroidManifest.xml`, along with various required permissions:

    <?xml version="1.0" encoding="utf-8"?>
    <manifest xmlns:android="http://schemas.android.com/apk/res/android"
              package="org.fourthline.cling.demo.android.browser">

        <uses-permission android:name="android.permission.INTERNET"/>
        <uses-permission android:name="android.permission.ACCESS_WIFI_STATE"/>
        <uses-permission android:name="android.permission.CHANGE_WIFI_MULTICAST_STATE"/>
        <uses-permission android:name="android.permission.ACCESS_NETWORK_STATE"/>
        <uses-permission android:name="android.permission.WAKE_LOCK"/>

        <uses-sdk
                android:targetSdkVersion="22"
                android:minSdkVersion="15"/>

        <application
                android:icon="@drawable/appicon"
                android:label="@string/appName"
                android:allowBackup="false">

            <activity android:name=".BrowserActivity">
                <intent-filter>
                    <action android:name="android.intent.action.MAIN"/>
                    <category android:name="android.intent.category.LAUNCHER"/>
                </intent-filter>
            </activity>

            <service android:name="org.fourthline.cling.android.AndroidUpnpServiceImpl"/>

            <!-- Or a custom service configuration, also use this class in bindService()!
            <service android:name=".BrowserUpnpService"/>
            -->

        </application>

    </manifest>

If a WiFi interface is present, Cling requires access to the interface. Cling will automatically detect when network interfaces are switched on and off and handle this situation gracefully: Any client operation will result in a "no response from server" state when no network is available. Your client code has to handle such a situation anyway.

Cling uses a custom configuration on Android, the `AndroidUpnpServiceConfiguration`, utilizing the Jetty transport and the `Recovering*` XML parsers and processors. See the Javadoc of the class for more information.

Jetty 8 libraries are required to use Cling on Android, see the demo applications for Maven dependencies!

For example, these dependencies are usually required in a Maven POM for Cling to work on Android:

The service component starts and stops the UPnP system when the service component is created and destroyed. This depends on how you access the service component from within your activities.

5.2. Accessing the service from an activity

The lifecycle of service components in Android is well defined. The first activity which binds to a service will start the service if it is not already running. When no activity is bound to the service any more, the operating system will destroy the service.

Let's write a simple UPnP browsing activity. It shows all devices on your network in a list and it has a menu option which triggers a search action. The activity connects to the UPnP service and then listens to any device additions or removals in the `Registry`, so the displayed list of devices is kept up-to-date:

    public class BrowserActivity extends ListActivity {

        private ArrayAdapter<DeviceDisplay> listAdapter;

        private BrowseRegistryListener registryListener = new BrowseRegistryListener();

        private AndroidUpnpService upnpService;

        private ServiceConnection serviceConnection = new ServiceConnection() {

            public void onServiceConnected(ComponentName className, IBinder service) {
                upnpService = (AndroidUpnpService) service;

                // Clear the list
                listAdapter.clear();

                // Get ready for future device advertisements
                upnpService.getRegistry().addListener(registryListener);

                // Now add all devices to the list we already know about
                for (Device device : upnpService.getRegistry().getDevices()) {
                    registryListener.deviceAdded(device);
                }

                // Search asynchronously for all devices, they will respond soon
                upnpService.getControlPoint().search();
            }

            public void onServiceDisconnected(ComponentName className) {
                upnpService = null;
            }
        };

        @Override
        public void onCreate(Bundle savedInstanceState) {
            super.onCreate(savedInstanceState);

            // Fix the logging integration between java.util.logging and Android internal logging
            org.seamless.util.logging.LoggingUtil.resetRootHandler(
                new FixedAndroidLogHandler()
            );
            // Now you can enable logging as needed for various categories of Cling:
            // Logger.getLogger("org.fourthline.cling").setLevel(Level.FINEST);

            listAdapter = new ArrayAdapter<>(this, android.R.layout.simple_list_item_1);
            setListAdapter(listAdapter);

            // This will start the UPnP service if it wasn't already started
            getApplicationContext().bindService(
                new Intent(this, AndroidUpnpServiceImpl.class),
                serviceConnection,
                Context.BIND_AUTO_CREATE
            );
        }

        @Override
        protected void onDestroy() {
            super.onDestroy();
            if (upnpService != null) {
                upnpService.getRegistry().removeListener(registryListener);
            }
            // This will stop the UPnP service if nobody else is bound to it
            getApplicationContext().unbindService(serviceConnection);
        }
        // ...
    }

We utilize the default layout provided by the Android runtime and the `ListActivity` superclass. Note that this activity can be your applications main activity, or further up in the stack of a task. The `listAdapter` is the glue between the device additions and removals on the Cling `Registry` and the list of items shown in the user interface.

Debug logging on Android

Cling uses the standard JDK logging, `java.util.logging`. Unfortunately, by default on Android you will not see `FINE`, `FINER`, and `FINEST` log messages, as their built-in log handler is broken (or, so badly designed that it might as well be broken). The easiest workaround is to set a custom log handler available in the `FixedAndroidLogHandler` class.

The `upnpService` variable is `null` when no backend service is bound to this activity. Binding and unbinding occurs in the `onCreate()` and `onDestroy()` callbacks, so the activity is bound to the service as long as it is alive.

Binding and unbinding the service is handled with the `ServiceConnection`: On connect, first a listener is added to the `Registry` of the UPnP service. This listener will process additions and removals of devices as they are discovered on your network, and update the items shown in the user interface list. The `BrowseRegistryListener` is removed when the activity is destroyed.

Then any already discovered devices are added manually to the user interface, passing them through the listener. (There might be none if the UPnP service was just started and no device has so far announced its presence.) Finally, you start asynchronous discovery by sending a search message to all UPnP devices, so they will announce themselves. This search message is NOT required every time you connect to the service. It is only necessary once, to populate the registry with all known devices when your (main) activity and application starts.

This is the `BrowseRegistryListener`, its only job is to update the displayed list items:

    protected class BrowseRegistryListener extends DefaultRegistryListener {

        /* Discovery performance optimization for very slow Android devices! */
        @Override
        public void remoteDeviceDiscoveryStarted(Registry registry, RemoteDevice device) {
            deviceAdded(device);
        }

        @Override
        public void remoteDeviceDiscoveryFailed(Registry registry, final RemoteDevice device, final Exception ex) {
            runOnUiThread(new Runnable() {
                public void run() {
                    Toast.makeText(
                        BrowserActivity.this,
                        "Discovery failed of '" + device.getDisplayString() + "': "
                            + (ex != null ? ex.toString() : "Couldn't retrieve device/service descriptors"),
                        Toast.LENGTH_LONG
                    ).show();
                }
            });
            deviceRemoved(device);
        }
        /* End of optimization, you can remove the whole block if your Android handset is fast (>= 600 Mhz) */

        @Override
        public void remoteDeviceAdded(Registry registry, RemoteDevice device) {
            deviceAdded(device);
        }

        @Override
        public void remoteDeviceRemoved(Registry registry, RemoteDevice device) {
            deviceRemoved(device);
        }

        @Override
        public void localDeviceAdded(Registry registry, LocalDevice device) {
            deviceAdded(device);
        }

        @Override
        public void localDeviceRemoved(Registry registry, LocalDevice device) {
            deviceRemoved(device);
        }

        public void deviceAdded(final Device device) {
            runOnUiThread(new Runnable() {
                public void run() {
                    DeviceDisplay d = new DeviceDisplay(device);
                    int position = listAdapter.getPosition(d);
                    if (position >= 0) {
                        // Device already in the list, re-set new value at same position
                        listAdapter.remove(d);
                        listAdapter.insert(d, position);
                    } else {
                        listAdapter.add(d);
                    }
                }
            });
        }

        public void deviceRemoved(final Device device) {
            runOnUiThread(new Runnable() {
                public void run() {
                    listAdapter.remove(new DeviceDisplay(device));
                }
            });
        }
    }

For performance reasons, when a new device has been discovered, we don't wait until a fully hydrated (all services retrieved and validated) device metadata model is available. We react as quickly as possible and don't wait until the `remoteDeviceAdded()` method will be called. We display any device even while discovery is still running. You'd usually not care about this on a desktop computer, however, Android handheld devices are slow and UPnP uses several bloated XML descriptors to exchange metadata about devices and services. Sometimes it can take several seconds before a device and its services are fully available. The `remoteDeviceDiscoveryStarted()` and `remoteDeviceDiscoveryFailed()` methods are called as soon as possible in the discovery process. On modern fast Android handsets, and unless you have to deal with dozens of UPnP devices on a LAN, you don't need this optimization.

By the way, devices are equal (`a.equals(b)`) if they have the same UDN, they might not be identical (`a==b`).

The `Registry` will call the listener methods in a separate thread. You have to update the displayed list data in the thread of the user interface.

The following methods on the activity add a menu with a search action, so a user can refresh the list manually:

Finally, the `DeviceDisplay` class is a very simple JavaBean that only provides a `toString()` method for rendering the list. You can display any information about UPnP devices by changing this method:

    protected class DeviceDisplay {

        Device device;

        public DeviceDisplay(Device device) {
            this.device = device;
        }

        public Device getDevice() {
            return device;
        }

        @Override
        public boolean equals(Object o) {
            if (this == o) return true;
            if (o == null || getClass() != o.getClass()) return false;
            DeviceDisplay that = (DeviceDisplay) o;
            return device.equals(that.device);
        }

        @Override
        public int hashCode() {
            return device.hashCode();
        }

        @Override
        public String toString() {
            String name =
                getDevice().getDetails() != null && getDevice().getDetails().getFriendlyName() != null
                    ? getDevice().getDetails().getFriendlyName()
                    : getDevice().getDisplayString();
            // Display a little star while the device is being loaded (see performance optimization earlier)
            return device.isFullyHydrated() ? name : name + " *";
        }
    }

We have to override the equality operations as well, so we can remove and add devices from the list manually with the `DeviceDisplay` instance as a convenient handle.

So far we have implemented a UPnP control point, next we create a UPnP device with services.

5.3. Creating a UPnP device

The following activity provides a UPnP service, the well known SwitchPower:1 with a BinaryLight:1 device:

    public class LightActivity extends Activity implements PropertyChangeListener {

        private AndroidUpnpService upnpService;

        private UDN udn = new UDN(UUID.randomUUID()); // TODO: Not stable!

        private ServiceConnection serviceConnection = new ServiceConnection() {

            public void onServiceConnected(ComponentName className, IBinder service) {
                upnpService = (AndroidUpnpService) service;

                LocalService<SwitchPower> switchPowerService = getSwitchPowerService();

                // Register the device when this activity binds to the service for the first time
                if (switchPowerService == null) {
                    try {
                        LocalDevice binaryLightDevice = createDevice();

                        Toast.makeText(LightActivity.this, R.string.registeringDevice, Toast.LENGTH_SHORT).show();
                        upnpService.getRegistry().addDevice(binaryLightDevice);

                        switchPowerService = getSwitchPowerService();

                    } catch (Exception ex) {
                        log.log(Level.SEVERE, "Creating BinaryLight device failed", ex);
                        Toast.makeText(LightActivity.this, R.string.createDeviceFailed, Toast.LENGTH_SHORT).show();
                        return;
                    }
                }

                // Obtain the state of the power switch and update the UI
                setLightbulb(switchPowerService.getManager().getImplementation().getStatus());

                // Start monitoring the power switch
                switchPowerService.getManager().getImplementation().getPropertyChangeSupport()
                        .addPropertyChangeListener(LightActivity.this);

            }

            public void onServiceDisconnected(ComponentName className) {
                upnpService = null;
            }
        };

        @Override
        public void onCreate(Bundle savedInstanceState) {
            super.onCreate(savedInstanceState);

            setContentView(R.layout.light);

            getApplicationContext().bindService(
                    new Intent(this, AndroidUpnpServiceImpl.class),
                    serviceConnection,
                    Context.BIND_AUTO_CREATE
            );
        }

        @Override
        protected void onDestroy() {
            super.onDestroy();

            // Stop monitoring the power switch
            LocalService<SwitchPower> switchPowerService = getSwitchPowerService();
            if (switchPowerService != null)
                switchPowerService.getManager().getImplementation().getPropertyChangeSupport()
                        .removePropertyChangeListener(this);

            getApplicationContext().unbindService(serviceConnection);
        }

        protected LocalService<SwitchPower> getSwitchPowerService() {
            if (upnpService == null)
                return null;

            LocalDevice binaryLightDevice;
            if ((binaryLightDevice = upnpService.getRegistry().getLocalDevice(udn, true)) == null)
                return null;

            return (LocalService<SwitchPower>)
                    binaryLightDevice.findService(new UDAServiceType("SwitchPower", 1));
        }
        // ...
    }

When the UPnP service is bound, for the first time, we check if the device has already been created by querying the `Registry`. If not, we create the device and add it to the `Registry`.

Generating a stable UDN on Android

The UDN of a UPnP device is supposed to be stable: It should not change between restarts of the device. Unfortunately, the Cling helper method `UDN.uniqueSystemIdentifier()` doesn't work on Android, see its Javadoc. Generating a new UUID every time your activity starts might be OK for testing, in production you should generate a UUID once when your application starts for the first time and store the UUID value in your application's preferences.

The activity is also a JavaBean `PropertyChangeListener`, registered with `SwitchPower` service. Note that this is JavaBean eventing, it has nothing to do with UPnP GENA eventing! We monitor the state of the service and switch the UI accordingly, turning the light on and off:

    public class LightActivity extends Activity implements PropertyChangeListener {

        public void propertyChange(PropertyChangeEvent event) {
            // This is regular JavaBean eventing, not UPnP eventing!
            if (event.getPropertyName().equals("status")) {
                log.info("Turning light: " + event.getNewValue());
                setLightbulb((Boolean) event.getNewValue());
            }
        }

        protected void setLightbulb(final boolean on) {
            runOnUiThread(new Runnable() {
                public void run() {
                    ImageView imageView = (ImageView) findViewById(R.id.light_imageview);
                    imageView.setImageResource(on ? R.drawable.light_on : R.drawable.light_off);
                    // You can NOT externalize this color into /res/values/colors.xml. Go on, try it!
                    imageView.setBackgroundColor(on ? Color.parseColor("#9EC942") : Color.WHITE);
                }
            });
        }
        // ...
    }

The `createDevice()` method simply instantiates a new `LocalDevice`:

    public class LightActivity extends Activity implements PropertyChangeListener {

        protected LocalDevice createDevice()
                throws ValidationException, LocalServiceBindingException {

            DeviceType type =
                    new UDADeviceType("BinaryLight", 1);

            DeviceDetails details =
                    new DeviceDetails(
                            "Friendly Binary Light",
                            new ManufacturerDetails("ACME"),
                            new ModelDetails("AndroidLight", "A light with on/off switch.", "v1")
                    );

            LocalService service =
                    new AnnotationLocalServiceBinder().read(SwitchPower.class);

            service.setManager(
                    new DefaultServiceManager<>(service, SwitchPower.class)
            );

            return new LocalDevice(
                    new DeviceIdentity(udn),
                    type,
                    details,
                    createDefaultDeviceIcon(),
                    service
            );
        }
        // ...
    }

For the `SwitchPower` class, again note the dual eventing for JavaBeans and UPnP:

    @UpnpService(
            serviceId = @UpnpServiceId("SwitchPower"),
            serviceType = @UpnpServiceType(value = "SwitchPower", version = 1)
    )
    public class SwitchPower {

        private final PropertyChangeSupport propertyChangeSupport;

        public SwitchPower() {
            this.propertyChangeSupport = new PropertyChangeSupport(this);
        }

        public PropertyChangeSupport getPropertyChangeSupport() {
            return propertyChangeSupport;
        }

        @UpnpStateVariable(defaultValue = "0", sendEvents = false)
        private boolean target = false;

        @UpnpStateVariable(defaultValue = "0")
        private boolean status = false;

        @UpnpAction
        public void setTarget(@UpnpInputArgument(name = "NewTargetValue") boolean newTargetValue) {
            boolean targetOldValue = target;
            target = newTargetValue;
            boolean statusOldValue = status;
            status = newTargetValue;

            // These have no effect on the UPnP monitoring but it's JavaBean compliant
            getPropertyChangeSupport().firePropertyChange("target", targetOldValue, target);
            getPropertyChangeSupport().firePropertyChange("status", statusOldValue, status);

            // This will send a UPnP event, it's the name of a state variable that sends events
            getPropertyChangeSupport().firePropertyChange("Status", statusOldValue, status);
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "RetTargetValue"))
        public boolean getTarget() {
            return target;
        }

        @UpnpAction(out = @UpnpOutputArgument(name = "ResultStatus"))
        public boolean getStatus() {
            return status;
        }
    }

5.4. Optimizing service behavior

The UPnP service consumes memory and CPU time while it is running. Although this is typically not an issue on a regular machine, this might be a problem on an Android handset. You can preserve memory and handset battery power if you disable certain features of the Cling UPnP service, or if you even pause and resume it when appropriate.

Furthermore, some Android handsets do not support multicast networking (HTC phones, for example), so you have to configure Cling accordingly on such a device and disable most of the UPnP discovery protocol.

5.4.1. Tuning registry maintenance

There are several things going on in the background while the service is running. First, there is the registry of the service and its maintenance thread. If you are writing a control point, this background registry maintainer is going to renew your outbound GENA subscriptions with remote services periodically. It will also expire and remove any discovered remote devices when the drop off the network without saying goodbye. If you are providing a local service, your device announcements will be refreshed by the registry maintainer and inbound GENA subscriptions will be removed if they haven't been renewed in time. Effectively, the registry maintainer prevents stale state on the UPnP network, so all participants have an up-to-date view of all other participants, and so on.

By default the registry maintainer will run every second and check if there is something to do (most of the time there is nothing to do, of course). The default Android configuration however has a default sleep interval of three seconds, so it is already consuming less background CPU time - while your application might be exposed to somewhat outdated information. You can further tune this setting by overriding the `getRegistryMaintenanceIntervalMillis()` in the `UpnpServiceConfiguration`. On Android, you have to subclass the service implementation to provide a new configuration:

    public class BrowserUpnpService extends AndroidUpnpServiceImpl {

        @Override
        protected UpnpServiceConfiguration createConfiguration() {
            return new AndroidUpnpServiceConfiguration() {

                @Override
                public int getRegistryMaintenanceIntervalMillis() {
                    return 7000;
                }

            };
        }
    }

Don't forget to now configure `BrowserUpnpService` in your `AndroidManifest.xml` instead of the original implementation. You also have to use this class when binding to the service in your activities instead of `AndroidUpnpServiceImpl`.

5.4.2. Pausing and resuming registry maintenance

Another more effective but also more complex optimization is pausing and resuming the registry whenever your activities no longer need the UPnP service. This is typically the case when an activity is no longer in the foreground (paused) or even no longer visible (stopped). By default any activity state change has no impact on the state of the UPnP service unless you bind and unbind from and to the service in your activities lifecycle callbacks.

In addition to binding and unbinding from the service you can also pause its registry by calling `Registry#pause()` when your activity's `onPause()` or `onStop()` method is called. You can then resume the background service maintenance (thread) with `Registry#resume()`, or check the status with `Registry#isPaused()`.

Please read the Javadoc of these methods for more details and what consequences pausing registry maintenance has on devices, services, and GENA subscriptions. Depending on what your application does, this rather minor optimization might not be worth dealing with these effects. On the other hand, your application should already be able to handle failed GENA subscription renewals, or disappearing remote devices!

5.4.3. Configuring discovery

The most effective optimization is selective discovery of UPnP devices. Although the UPnP service's network transport layer will keep running (threads are waiting and sockets are bound) in the background, this feature allows you to drop discovery messages selectively and quickly.

For example, if you are writing a control point, you can drop any received discovery message if it doesn't advertise the service you want to control - you are not interested in any other device. On the other hand if you only provide devices and services, all discovery messages (except search messages for your services) can probably be dropped, you are not interested in any remote devices and their services at all.

Discovery messages are selected and potentially dropped by Cling as soon as the UDP datagram content is available, so no further parsing and processing is needed and CPU time/memory consumption is significantly reduced while you keep the UPnP service running even in the background on an Android handset.

To configure which services are supported by your control point application, override the configuration and provide an array of `ServiceType` instances:

    public class BrowserUpnpService extends AndroidUpnpServiceImpl {

        @Override
        protected UpnpServiceConfiguration createConfiguration() {
            return new AndroidUpnpServiceConfiguration() {

                @Override
                public ServiceType[] getExclusiveServiceTypes() {
                    return new ServiceType[]{
                        new UDAServiceType("SwitchPower")
                    };
                }
            };
        }
    }

This configuration will ignore any advertisement from any device that doesn't also advertise a schemas-upnp-org:SwitchPower:1 service. This is what our control point can handle, so we don't need anything else. If instead you'd return an empty array (the default behavior), all services and devices will be discovered and no advertisements will be dropped.

If you are not writing a control point but a server application, you can return `null` in the `getExclusiveServiceTypes()` method. This will disable discovery completely, now all device and service advertisements are dropped as soon as they are received.

6. Advanced options
6.1. Custom client/server information

Sometimes your service has to implement different procedures depending on the client who makes the action request, or you want to send a request with some identifying information about your client.

6.1.1. Adding extra request headers

By default, Cling will add all necessary headers to all outbound request messages. For HTTP-based messages such as descriptor retrieval, action invocation, and GENA messages, the `User-Agent` HTTP header will be set to a default value, obtained from your `StreamClientConfiguration`.

You can override this behavior for descriptor retrieval and GENA subscription messages with a custom configuration. For example, this configuration will send extra HTTP headers when device and service descriptors have to be retrieved for a particular UDN:

For GENA subscription, renewal, and unsubscribe messages, you can set extra headers depending on the service you are subscribing to:

For action invocations to remote services, you can set custom headers when constructing the `ActionInvocation`:

Any of these settings only affect outbound request messages! Any outbound response to a remote request will have only headers required by the UPnP protocols. See the next section on how to customize response headers for remote action requests.

Very rarely you have to customize SSDP (MSEARCH and its response) messages. First, subclass the default `ProtocolFactoryImpl` and override the instantiation of the protocols as necessary. For example, override `createSendingSearch()` and return your own instance of the `SendingSearch` protocol. Next, override `prepareOutgoingSearchRequest(OutgoingSearchRequest)` of the `SendingSearch` protocol and modify the message. The same procedure can be applied to customize search responses with the `ReceivingSearch` protocol.

6.1.2. Accessing remote client information

Theoretically, your service implementation should work with any client, as UPnP is supposed to provide a compatibility layer. In practice, this never works as no UPnP client and server is fully compatible with the specifications (except Cling, of course).

If your action method has a last (or only parameter) of type `RemoteClientInfo`, Cling will provide details about the control point calling your service:

    @UpnpAction
    public void setTarget(@UpnpInputArgument(name = "NewTargetValue")
                          boolean newTargetValue,
                          RemoteClientInfo clientInfo) {
        power = newTargetValue;
        System.out.println("Switch is: " + power);

        if (clientInfo != null) {
            System.out.println(
                "Client's address is: " + clientInfo.getRemoteAddress()
            );
            System.out.println(
                "Received message on: " + clientInfo.getLocalAddress()
            );
            System.out.println(
                "Client's user agent is: " + clientInfo.getRequestUserAgent()
            );
            System.out.println(
                "Client's custom header is: " +
                clientInfo.getRequestHeaders().getFirstHeader("X-MY-HEADER")
            );

            // Return some extra headers in the response
            clientInfo.getExtraResponseHeaders().add("X-MY-HEADER", "foobar");
        }
    }

The `RemoteClientInfo` argument will only be available when this action method is processing a remote client call, an `ActionInvocation` executed by the local UPnP stack on a local service does not have remote client information and the argument will be `null`.

A client's remote and local address might be `null` if the Cling transport layer was not able to obtain the connection's address.

You can set extra response headers on the `RemoteClientInfo`, which will be returned to the client with the response of your UPnP action. There is also a `setResponseUserAgent()` method for your convenience.

The `RemoteClientInfo` is also useful if you have to deal with potentially long-running actions.

6.2. Long-running actions

An action of a service might take a long time to complete and consume resources. For example, if your service has to process significant amounts of data, you might want to stop processing when the client calling your action is actually no longer connected. On the client side, you might want to give your users the option to interrupt and abort action requests if the service takes too long to respond. These are two distinct issues, and we'll first look at it from the client's perspective.

6.2.1. Cancelling an action invocation

You call actions of services with the `ControlPoint#execute(myCallback)` method. So far you probably haven't considered the optional return value of this method, a `Future` which can be used to cancel the invocation:

    Future future = upnpService.getControlPoint().execute(setTargetCallback);
    Thread.sleep(500);
    future.cancel(true);

Here we are calling the `SetTarget` action of a SwitchPower:1 service, and after waiting a (short) time period, we cancel the request. What happens now depends on the invocation and what service you are calling. If it's a local service, and no network access is needed, the thread calling the local service (method) will simply be interrupted. If you are calling a remote service, Cling will abort the HTTP request to the server.

Most likely you want to handle this explicit cancellation of an action call in your action invocation callback, so you can present the result to your user. Override the `failure()` method to handle the interruption:

    ActionCallback setTargetCallback = new ActionCallback(setTargetInvocation) {

        @Override
        public void success(ActionInvocation invocation) {
            // Will not be called if invocation has been cancelled
        }

        @Override
        public void failure(ActionInvocation invocation,
                            UpnpResponse operation,
                            String defaultMsg) {
            if (invocation.getFailure() instanceof ActionCancelledException) {
                // Handle the cancellation here...
            }
        }
    };

A special exception type is provided if the action call was indeed cancelled.

Several important issues have to be considered when you try to cancel action calls to remote services:

There is no guarantee that the server will actually stop processing your request. When the client closes the connection, the server doesn't get notified. The server will complete the action call and only fail when trying to return the response to the client on the closed connection. Cling's server transports offer a special heartbeat feature for checking client connections, we'll discuss this feature later in this chapter. Other UPnP servers will most likely not detect a dropped client connection immediately.

Not all HTTP client transports in Cling support interruption of requests:

Transport | Supports Interruption?
--- | ---
`org.fourthline.cling.transport.impl.StreamClientImpl (default)` | NO
`org.fourthline.cling.transport.impl.apache.StreamClientImpl` | YES
`org.fourthline.cling.transport.impl.jetty.StreamClientImpl (default on Android)` | YES

Transports which do not support cancellation won't produce an error when you abort an action invocation, they silently ignore the interruption and continue waiting for the server to respond.

6.2.2. Reacting to cancellation on the server

By default, an action method of your service will run until it completes, it either returns or throws an exception. If you have to perform long-running tasks in a service, your action method can avoid doing unnecessary work by checking if processing should continue. Think about processing in batches: You work for a while, then you check if you should continue, then you work some more, check again, and so on.

There are two checks you have to perform:

- If a local control point called your service, and meanwhile cancelled the action call, the thread running your action method will have its interruption flag set. When you see this flag you can stop processing, as any result of your action method will be ignored anyway.
- If a remote control point called your service, it might have dropped the connection while you were processing data to return. Unfortunately, checking if the client's connection is still open requires, on a TCP level, writing data on the socket. This is essentially a heartbeat signal: Every time you check if the client is still there, a byte of (hopefully) insignificant data will be send to the client. If there wasn't any error sending data, the connection is still alive.

These checks look as follows in your service method:

    @UpnpAction
    public void setTarget(@UpnpInputArgument(name = "NewTargetValue") boolean newTargetValue,
                          RemoteClientInfo remoteClientInfo) throws InterruptedException {

        boolean interrupted = false;
        while (!interrupted) {
            // Do some long-running work and periodically test if you should continue...

            // ... for local service invocation
            if (Thread.interrupted())
                interrupted = true;

            // ... for remote service invocation
            if (remoteClientInfo != null && remoteClientInfo.isRequestCancelled())
                interrupted = true;
        }
        throw new InterruptedException("Execution interrupted");
    }

You abort processing by throwing an `InterruptedException`, Cling will do the rest. Cling will send a heartbeat to the client whenever you check if the remote request was cancelled with the optional `RemoteClientInfo`, see this section.

Danger: Not all HTTP clients can deal with Cling's heartbeat signal. Not even all bundled `StreamClient`'s of Cling can handle such a signal. You should only use this feature if you are sure that all clients of your service will ignore the meaningless heartbeat signal. Cling sends a space character (this is configurable) to the HTTP client to check the connection. Hence, the HTTP client sees a response such as '[space][space][space]HTTP/1.0', with a space character for each alive check. If your HTTP client does not trim those space characters before parsing the response, it will fail processing your otherwise valid response.

The following Cling-bundled client transports can deal with a heartbeat signal:

Transport | Accepts Heartbeat?
--- | ---
`org.fourthline.cling.transport.impl.StreamClientImpl (default)` | NO
`org.fourthline.cling.transport.impl.apache.StreamClientImpl` | YES
`org.fourthline.cling.transport.impl.jetty.StreamClientImpl (default on Android)` | YES

Equally important, not all server transports in Cling can send heartbeat signals, as low-level socket access is required. Some server APIs do not provide this low-level access. If you check the connection state with those transports, the connection is always "alive":

Transport | Sends Heartbeat?
--- | ---
`org.fourthline.cling.transport.impl.StreamServerImpl (default)` | NO
`org.fourthline.cling.transport.impl.apache.StreamServerImpl` | YES
`org.fourthline.cling.transport.impl.AsyncServletStreamServerImpl` with `org.fourthline.cling.transport.impl.jetty.JettyServletContainer (default on Android)` | YES

In practice, this heartbeat feature is less useful than it sounds in theory: As you usually don't control which HTTP clients will access your server, sending them "garbage" bytes before responding properly will most likely cause interoperability problems.

6.3. Switching XML descriptor binders

UPnP utilizes XML documents to transport device and service information between the provider and any control points. These XML documents have to be parsed by Cling to produce the `Device` model, and of course generated from a `Device` model. The same approach is used for the `Service` model. This parsing, generating, and binding is the job of the `org.fourthline.cling.binding.xml.DeviceDescriptorBinder` and the `org.fourthline.cling.binding.xml.ServiceDescriptorBinder`.

The following implementations are bundled with Cling Core for device descriptor binding:

`org.fourthline.cling.binding.xml.UDA10DeviceDescriptorBinderImpl` (default)
  This implementation reads and writes UDA 1.0 descriptor XML with the JAXP-provided DOM API provided by JDK 6. You do not need any additional libraries to use this binder. Use this binder to validate strict specification compliance of your applications.
`org.fourthline.cling.binding.xml.UDA10DeviceDescriptorBinderSAXImpl`
  This implementation reads and writes UDA 1.0 descriptor XML with the JAXP-provided SAX API, you don't have to install additional libraries to use it. This binder may consume less memory when reading XML descriptors and perform better than the DOM-based parser. In practice, the difference is usually insignificant, even on very slow machines.
`org.fourthline.cling.binding.xml.RecoveringUDA10DeviceDescriptorBinderImpl`
  This implementation extends `UDA10DeviceDescriptorBinderImpl` and tries to recover from parsing failures, and works around known problems of other UPnP stacks. This is the binder you want for best interoperability in real-world UPnP applications. Furthermore, you can override the `handleInvalidDescriptor()` and `handleInvalidDevice()` methods to customize error handling, or if you want to repair invalid device information manually. It is the default binder for `AndroidUpnpServiceConfiguration`.

The following implementations are bundled with Cling Core for service descriptor binding:

`org.fourthline.cling.binding.xml.UDA10ServiceDescriptorBinderImpl` (default)
  This implementation reads and writes UDA 1.0 descriptor XML with the JAXP-provided DOM API provided by JDK 6. You do not need any additional libraries to use this binder. Use this binder to validate strict specification compliance of your applications.
`org.fourthline.cling.binding.xml.UDA10ServiceDescriptorBinderSAXImpl`
  This implementation reads and writes UDA 1.0 descriptor XML with the JAXP-provided SAX API, you don't have to install additional libraries to use it. This binder may consume less memory when reading XML descriptors and perform better than the DOM-based parser. In practice, the difference is usually insignificant, even on very slow machines. It is the default binder for `AndroidUpnpServiceConfiguration`.

You can switch descriptor binders by overriding the `UpnpServiceConfiguration`:

Performance problems with UPnP discovery are usually caused by too many XML descriptors, not by their size. This is inherent in the bad design of UPnP; each device may expose many individual service descriptors, and Cling will always retrieve all device metadata. The HTTP requests necessary to retrieve dozens of descriptor files usually outweighs the cost of parsing each.

Note that binders are only used for device and service descriptors, not for UPnP action and event message processing.

6.4. Switching XML processors

All control and event UPnP messages have an XML payload, and the control messages are even wrapped in SOAP envelopes. Handling XML for control and eventing is encapsulated in the Cling transport layer, with an extensible service provider interface:

`org.fourthline.cling.transport.spi.SOAPActionProcessor`
  This processor reads and writes UPnP SOAP messages and transform them from/to `ActionInvocation` data. The protocol layer, on top of the transport layer, handles `ActionInvocation` only.
`org.fourthline.cling.transport.spi.GENAEventProcessor`
  This processor reads and writes UPnP GENA event messages and transform them from/to a `List<StateVariableValue>`.

For the `SOAPActionProcessor`, the following implementations are bundled with Cling Core:

`org.fourthline.cling.transport.impl.SOAPActionProcessorImpl` (default)
  This implementation reads and writes XML with the JAXP-provided DOM API provided by JDK 6. You do not need any additional libraries to use this processor. However, its strict compliance with the UPnP specification can cause problems in real-world UPnP applications. This processor will produce errors during reading when XML messages violate the UPnP specification. Use it to test a UPnP stack or application for strict specification compliance.
`org.fourthline.cling.transport.impl.PullSOAPActionProcessorImpl`
  This processor uses the XML Pull API to read messages, and the JAXP DOM API to write messages. You need an implementation of the XML Pull API on your classpath to use this processor, for example, XPP3 or kXML 2. Compared with the default processor, this processor is much more lenient when reading action message XML. It can deal with broken namespacing, missing SOAP envelopes, and other problems. In UPnP applications where interoperability is more important than specification compliance, you should use this parser.
`org.fourthline.cling.transport.impl.RecoveringSOAPActionProcessorImpl`
  This processor extends the `PullSOAPActionProcessorImpl` and additionally will work around known bugs of UPnP stacks in the wild and try to recover from parsing failures by modifying the XML text in different ways. This is the processor you should use for best interoperability with other (broken) UPnP stacks. Furthermore, it let's you handle a failure when reading an XML message easily by overriding the `handleInvalidMessage()` method, e.g. to create or log an error report. It is the default processor for `AndroidUpnpServiceConfiguration`.

For the `GENAEventProcessor`, the following implementations are bundled with Cling Core:

`org.fourthline.cling.transport.impl.GENAEventProcessorImpl` (default)
  This implementation reads and writes XML with the JAXP-provided DOM API provided by JDK 6. You do not need any additional libraries to use this processor. However, its strict compliance with the UPnP specification can cause problems in real-world UPnP applications. This processor will produce errors during reading when XML messages violate the UPnP specification. Use it to test a UPnP stack or application for strict specification compliance.
`org.fourthline.cling.transport.impl.PullGENAEventProcessorImpl`
  This processor uses the XML Pull API to read messages, and the JAXP DOM API to write messages. You need an implementation of the XML Pull API on your classpath to use this processor, for example, XPP3 or kXML 2. Compared with the default processor, this processor is much more lenient when reading action message XML. It can deal with broken namespacing, missing root element, and other problems. In UPnP applications where compatibility is more important than specification compliance, you should use this parser.
`org.fourthline.cling.transport.impl.RecoveringGENAEventProcessorImpl`
  This processor extends the `PullGENAEventProcessorImpl` and additionally will work around known bugs of UPnP stacks in the wild and try to recover from parsing failures by modifying the XML text in different ways. This is the processor you should use for best interoperability with other (broken) UPnP stacks. Furthermore, it will return partial results, when at least one single state variable value was successfully read from the event XML. It is the default processor for `AndroidUpnpServiceConfiguration`.

You can switch XML processors by overriding the `UpnpServiceConfiguration`:

6.5. Solving discovery problems

Device discovery in UPnP is the job of SSDP, the Simple Service Discovery Protocol. Of course, this protocol is not simple at all and many device manufacturers and UPnP stacks get it wrong. Cling has some extra settings to deal with such environments; if you want best interoperability for your application, you have to read the following sections.

6.5.1. Maximum age of remote devices

If you are writing a control point and remote devices seem to randomly disappear from your `Registry`, you are probably dealing with a remote device that doesn't send regular alive NOTIFY heartbeats through multicast. Or, your control point runs on a device that doesn't properly receive multicast messages. (Android devices from HTC are known to have this issue.)

Cling will usually expire remote devices once their initially advertised "maximum age" has been reached and there was no ALIVE message to refresh the advertisement. You can change this behavior with `UpnpServiceConfiguration`:

If you return zero maximum age, all remote devices will forever stay in your `Registry` once they have been discovered, Cling will not expire them. You have to manually remove them from the `Registry` if you know they are gone (e.g. once an action request fails with "no response").

Alternatively, you can return the number of seconds Cling should keep a remote device in the `Registry`, ignoring the device's advertised maximum age.

6.5.2. Alive messages at regular intervals

Some control points have difficulties with M-SEARCH responses. They search for your device, then can't process the (specification-compliant) response made by Cling and therefore don't discover your device when they search. However, such control points typically have no problem with alive NOTIFY messages, only with search responses.

The solution then is to repeat alive NOTIFY messages for all your local devices on the network very frequently, let's say every 5 seconds:

By default this method returns `0`, disabling alive message flooding and relying on the regular triggering of local device advertisements (which depends on the maximum age of each `LocalDeviceIdentity`).

If you return a non-zero value, Cling will send alive NOTIFY messages repeatedly with the given interval, and remote control points should be able to discover your device within that period. The downside is of course more traffic on your network.

6.5.3. Using discovery options for local devices

If you create a `LocalDevice` that you don't want to announce to remote control points, add it to the `Registry` with `addDevice(localDevice, new DiscoveryOptions(false))`.

The `DiscoveryOptions` class offers several parameters to influence how Cling handles device discovery.

With disabled advertising, Cling will then not send any NOTIFY messages for a device; you can enable advertisement again with `Registry#setDiscoveryOptions(UDN, null)`, or by providing different options.

Note that remote control points will still be able to discover your device if they know your device descriptor URL. They will also be able to call actions and subscribe to services. This is not a switch to make a `LocalDevice` "private", it only disables (multicast) advertising.

A rarely used setting of `DiscoveryOptions` is `byeByeBeforeFirstAlive`: If enabled, Cling will send a byebye NOTIFY message before sending the first alive NOTIFY message. This happens only once, when a `LocalDevice` is added to the `Registry`, and it wasn't registered before.

6.5.4. Manual advertisement of local devices

You can force immediate advertisement of all registered `LocalDevice`s with `Registry#advertiseLocalDevices()`. Note that no announcements will be made for any device with disabled advertising (see previous section).

6.6. Configuring network transports

Cling has to accept and make HTTP requests to implement UPnP discovery, action processing, and GENA eventing. This is the job of the `StreamServer` and `StreamClient` implementations, working together with the `Router` as the Cling network transport layer.

For the `StreamClient` SPI, the following implementations are bundled with Cling:

`org.fourthline.cling.transport.impl.StreamClientImpl` (default)
  This implementation uses the JDK's `HTTPURLConnection`, it doesn't require any additional libraries. Note that Cling has to customize (with an ugly hack, really) the VM's `URLStreamHandlerFactory` to support additional HTTP methods such as `NOTIFY`, `SUBSCRIBE`, and `UNSUBSCRIBE`. The designers of the JDK do not understand HTTP very well and made this extremely difficult to extend. Cling's patch only works if no other code in your environment has already set a custom `URLStreamHandlerFactory`, you will get an exception on startup if this issue is detected; then you have to switch to another `StreamClient` implementation. Note that this implementation does NOT WORK on Android, the `URLStreamHandlerFactory` can't be patched on Android!
`org.fourthline.cling.transport.impl.jetty.StreamClientImpl`
  This implementation is based on the Jetty 8 HTTP client, you need the artifact `org.eclipse.jetty:jetty-client:8.1` on your classpath to use it. This implementation works in any environment, including Android. It is the default transport for `AndroidUpnpServiceConfiguration`.

For the `StreamServer` SPI, the following implementations are bundled with Cling:

`org.fourthline.cling.transport.impl.StreamServerImpl` (default)
  This implementation uses the built-in webserver of the Sun JDK 6 (`com.sun.net.httpserver.HttpServer`), hence, it does NOT WORK in an Android environment.
`org.fourthline.cling.transport.impl.AsyncServletStreamServerImpl`
  This implementation is based on the standard Servlet 3.0 API and can be used in any environment with a compatible servlet container. It requires a `ServletContainerAdapter` to integrate with the servlet container, the bundled `JettyServletContainer` is such an adapter for a standalone Jetty 8 server. You need the artifact `org.eclipse.jetty:jetty-servlet:8.1` on your classpath to use it. This implementation works in any environment, including Android. It is the default transport for `AndroidUpnpServiceConfiguration`. For other containers, write your own adapter and provide it to the `AsyncServletStreamServerConfigurationImpl`.

Each `StreamClient` and `StreamServer` implementation is paired with an implementation of `StreamClientConfiguration` and `StreamServerConfiguration`. This is how you override the Cling network transport configuration:

The above configuration will use the Jetty client and the Jetty servlet container. The `JettyServletContainer.INSTANCE` adapter is managing a standalone singleton server, it is started and stopped when Cling starts and stops the UPnP stack. If you have run Cling with an existing, external servlet container, provide a custom adapter.

This manual has been created with Lemma from tested source code and Javadoc. Try it, you will like it.