## Uses of Interface
org.fourthline.cling.model.Validatable

- Packages that use Validatable
  Package | Description
  --- | ---
  org.fourthline.cling.model.meta |

- - ### Uses of Validatable in org.fourthline.cling.model.meta

    Classes in org.fourthline.cling.model.meta that implement Validatable
    Modifier and Type | Class and Description
    --- | ---
    `class` | `Action<S extends Service>` Describes an action and its input/output arguments.
    `class` | `ActionArgument<S extends Service>` Describes a single action argument, either input or output.
    `class` | `Device<DI extends DeviceIdentity,D extends Device,S extends Service>` Describes either a root or embedded device.
    `class` | `DeviceDetails` Encapsulates all optional metadata about a device.
    `class` | `DeviceIdentity` Unique device name, received and offered during discovery with SSDP.
    `class` | `Icon` The metadata of a device icon, might include the actual image data of a local icon.
    `class` | `LocalDevice` The metadata of a device created on this host, by application code.
    `class` | `QueryStateVariableAction<S extends Service>` Describes a single action, the deprecated "query any state variable" action.
    `class` | `RemoteDevice` The metadata of a device that was discovered on the network.
    `class` | `RemoteDeviceIdentity` Additional identifying information only relevant for discovered remote devices.
    `class` | `StateVariable<S extends Service>` The metadata of a named state variable.
    `class` | `StateVariableAllowedValueRange` Integrity rule for a state variable, restricting its values to a range with steps.
    `class` | `StateVariableTypeDetails` Type of a state variable, its default value, and integrity rules for allowed values and ranges.
    `class` | `UDAVersion` Version of the UPnP Device Architecture (UDA), defaults to 1.0.

Copyright © 2016 4th Line GmbH, Switzerland. All rights reserved.